00 Select Maker
01 Select Driver
02 Device USB not found
03 Low Speed
04 ECU Data
05 Read ECU
06 Open File
07 Download File
08 Exit
09 ECU Data
10 Commands
11 Programming Data File
12 USB Device Active 
13 USB Device Not Active 
14 Opening USB port impossible 
15 Opening port impossible 
16 Wait...
17 Turn On Dashboard
18 File not compressed
19 TURN OFF AND TURN ON THE DASHBOARD BEFORE READ OR WRITE ECU
20 ATTENTION: BEFORE PROGRAMMING SET PIN 10/8 ECU TO 12V AND CHECK THAT THE TENSION IS AT LEAST Of 13 V
21 READING TIME: 30 minuts CONTINUE ?
22 First select a driver
23 First open a file
24 not exist
25 END OF READ. TURN OF THE DASHBOARD
26 TURN 10sec OFF AND TURN ON THE DASHBOARD WAIT 10Sec BEFORE OF CONTINUE
27 error writing file
28 no file open
29 error writing
30 impossible erase ECU
31 inactive port
32 ECU not selected
33 comunication impossible
34 Writing Initilization
35 READING ECU 
36 Start reading...
37 Closing ECU...
38 Start writing...
39 Erasing... 
40 WRITING ECU
41 WRONG FILE DIMENSION
42 reading error or wrong file dimension
43 reading error
44 changing speed error
45 impossible initialize writing
46 ECU NUMBER NOT FOUND
47 Data reading error
48 ECU erased
49 writing error
50 max number of erasing tries exceeded
51 ECU coded
52 ECU not coded
53 operation cancelled 
54 TURN OFF AND TURN ON THE DASHBOARD. READING DATA TIME: 2 MINUTES. CONTINUE ?
55 ATTENTION: BEFORE PROGRAMMING SET PIN "B3" ECU TO 12V AND CHECK THAT THE TENSION IS AT LEAST Of 13 V
56 High Speed
57 Cars
58 DATA READING
59 Start data reading...
60 COMPLETE
61 TABLES
62 ATTENTION BEFORE TO CONTINUE: REMOVE FEEDING,  PUT  PIN 24 FLASH EPROM TO MASS, GIVE FEEDING AND REMOVE TO MASS PIN 24 FLASH, END TO CONTINUE.SEE THE PDF FILE IN FOLDER DOCUMENTI
63 ATTENTION BEFORE TO CONTINUE: REMOVE THE FUSE N°11, PUT IL PIN 24 FLASH EPROM To MASS, GIVE FEEDING AND REMOVE TO MASS PIN 24 FLASH, END TO CONTINUE.
64 TURN ON THE DASHBOARD END REMOVE THE FUSE N°11 AFTER 5 S,END TO CONTINUE.
65 OFF THE DASHBOARD, INSERT FHE FUSE N°11, TURN ON THE DASHBOARD, END REMOVE THE FUSE N°11 AFTER 5 S,END TO CONTINUE.
66 ATTENTION BEFORE TO CONTINUE: REMOVE FEEDING,  PUT  PIN 28 FLASH EPROM TO MASS, GIVE FEEDING AND REMOVE TO MASS PIN 28 FLASH, END TO CONTINUE.SEE THE PDF FILE IN FOLDER DOCUMENTI
67 READING TIME FILE wHOLE: 1 HOUR. CONTINUE ?
68 ATTENTION BEFORE TO CONTINUE: REMOVE FEEDING,  PUT PIN 104 POL.4 MICRO TO MASS, GIVE FEEDING AND REMOVE TO MASS PIN 104 POL.4 MICRO, END TO CONTINUE.SEE THE PDF FILE IN FOLDER DOCUMENTI
69 ATTENTION BEFORE WRITE SET PIN 64 ECU TO 12V AND CHECK THAT THE TENSION IS AT LEAST Of 13 V
70 BOOT MODE INACTIVE
71 FILE WRONG
72 MICRO MOTOROLA NOT SUPPORTED
73 ATTENTION BEFORE TO READING OR VRITE : REMOVE FEEDING PUT PIN 20 ECU TO MASS, GIVE FEEDING END TO CONTINUE.SEE THE PDF FILE IN FOLDER DOCUMENTI
74 ATTENTION BEFORE READ OR WRITE CHECK THAT THE TENSION IS AT LEAST Of 13 V
75 ATTENZION  IF YOU MUST NOT COMMUNICATE MAKE  A BRIDGE BETWEEN IL PIN 7 > 11  EOBD2 PLUG
76 ATTENTION FOR COMMUNICATE Us WITH THIS VEHICLE YOU WANTS ADAPTER TO 24V, OR CUT 1 OF THE 2 BATTERIES To 12V
77 TURN OFF THE DASHBOARD AND START THE ENGINE
78 ATTENTION FOR EXTINGUISH SPY MOTOR AFTER THE PROGRAMM PERFORM 3 TIMES DATI ECU
79 ATTENTION IF YOU MUST NOT COMMUNICATE CONNECT  PIN 7 Kline OF THE EOBD TO PIN 72 Kline ECU ENGINE
80 ATTENTION IF YOU MUST NOT COMMUNICATE CONNECT  PIN 7 Kline OF THE EOBD TO PLUG 2 PIN 43 Kline ECU ENGINE
81 ATTENTION BEFORE TO READING: REMOVE FEEDING PUT TO MASS WITH THE PICTURE IN FOLDER DUCUMENT *.jpg, AND REMOVE MASS, GIVE FEEDING END TO CONTINUE.SEE THE PDF FILE IN FOLDER DOCUMENTI
82 ATTENTION IF YOU MUST NOT COMMUNICATE CONNECT  PIN 7 Kline OF THE EOBD TO PLUG K PIN 25 Kline ECU ENGINE
83 BEGINNING 2° ECU SLAVE, OK ?
84 ATTENTION, SAVED 2 FILES, YOU 2 ECUS IS DIFFERENT, THEY COULD NOT BE WRITTEN
85 ATTENTION BEFORE WRITE LINK RELAIS SEE *.PDF IN DOCUMENTS, AND CHECK THAT THE TENSION IS AT LEAST Of 13 V
86 ATTENTION BEFORE PROCEED: REMOVE CURRENT, OPEN ECU AND PERFORM A LINK WITH A THREAD, LOOK AT FIGURE In DOCUMENTS* .jpg, GIVE CURRENT, GIVE "OK," AFTER REMOVE AND GIVE CURRENT QUICKLY ON ECU.
87 ATTENTION REMOVE MASS AND PROCEED GIVING "OK".
88 CHK COMPUTED IN WRITING
89 TURN OFF AND TURN ON THE DASHBOARD AND TRY AGAIN
90 IF THERE'S NO RESPONSE CONNECT PIN 7 OF EOBD2 TO PIN B4 OF 32_PIN BLACK IN ECU
91 RSA NOT RECOGNIZED
92 ATTENTION IF YOU MUST NOT COMMUNICATE CONNECT  PIN 7 Kline OF THE EOBD TO PIN 86 Kline ECU ENGINE