CATEGORY=Parameters\Extras\IAB Activation

PAGE_DESCRIPTION_START_HERE

IMG1=helpIAB.png

LABEL1=
IAB Output will turn off the activation changes of the output.

Engage is the RPM the IABs will open.

Disengage is the RPM the IABs will close.

USDM ECU is used to tell the ECU which output to use.
It is different on JDM/USDM ECUs.
!LABEL1