

![board](installations/MazdaMiataNA6_Frankenso_pnp/Frankenso_MazdaMiataNA6_pnp_053_na6_v0_1.jpg)

[Frankenso Board Technical Details](https://rusefi.com/wiki/index.php?title=Manual:Hardware_Frankenso_board#Default_Pinout)

| # & Color | From | To | Function |   |
|------|------|----|-------|---|
| #1 White L=75mm    | 3E plug / top of W43  |               | crank angle sensor   |   |
| #2 Yellow L=75mm   | 3G plug / top of W45  |               | crank angle sensor   |   |
| #3 White L=160mm   | 1E plug / top of W4   | bottom W62    | check Engine     |   | 
| #4 Red L=90mm      | 2F plug / top of W28  | top of W49    | external MAP +5v power     |   |
| #5 Green L=90mm    | 2E plug / top of W27  | bottom W47    | external MAP signal      |   |
| #6 Black L=60mm    | 2N plug / top of W36  | top of W40    | external MAP ground      |   |
| #7 Blue L=75mm     | 2I plug / top of W31  | W52           | external wide band oxygen sensor signal |
| #8 Black L=60mm    | 2M plug / top of W35  | top of W39    | external wide band oxygen sensor ground      |
| #9 Green L=120mm   | 1Q plug / top of W17  | bottom of W46 | A/C switch input |
| #10                | 1J plug /             | .             | A/C relay output  |
| #11 Yellow L=120mm | 1V plug / top of W22  | bottom of W48 | clutch pedal switch  |
|      |      |    |       |   |
|      |      |    |       |   |
| 30V 0.5A Schottky Diode (for example RSX051VYM30FHTR)     | top of ?    | bottom of ?   | Idle Air Valve fly-back diode      |   |
|      |      |    |       |   |

-----------------------------------
