

TODO :)

See https://rusefi.com/forum/viewtopic.php?f=5&t=592&start=150#p32044

tl;dr:

1) Zero out PID gains, adjust bias table to cancel out the spring

2) Tune PID


See also https://rusefi.com/s/debugmode/