(footprint "vr-discrete" (version 20210424) (generator pcbnew) (layer "F.Cu")
  (tedit 609C1979)
  (fp_text reference "REF**" (at 2.38 -15.86 unlocked) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3bbb3196-d395-42e9-93c4-2cfa30650db5)
  )
  (fp_text value "M750" (at 9.02 -16 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c336454c-aae3-4dad-89cd-9cf802b33056)
  )
  (fp_rect (start 18.15 -16.85) (end 0.1 -0.1) (layer "B.SilkS") (width 0.2) (fill none) (tstamp c71593d3-44a3-4dc7-aaf0-1a37b8b2fab0))
  (fp_rect (start 18.15 -16.85) (end 0.1 -0.1) (layer "F.SilkS") (width 0.2) (fill none) (tstamp b1d3ac64-b6a3-45b5-9e8e-ad509bc8209b))
  (pad "E1" thru_hole circle locked (at 17.9 -0.875 180) (size 0.599999 0.599999) (drill 0.299999) (layers *.Cu *.Mask)
    (solder_paste_margin -49.999999) (zone_connect 2) (tstamp 06a906cd-f5c2-467f-9906-e39ae0e9a54d))
  (pad "E2" thru_hole circle locked (at 17.9 -8.375 180) (size 0.599999 0.599999) (drill 0.299999) (layers *.Cu *.Mask)
    (solder_paste_margin -49.999999) (zone_connect 2) (tstamp 7a29b1ba-b8a3-483a-8274-fd49b8f68e66))
  (pad "E3" thru_hole circle locked (at 17.9 -9.175 180) (size 0.599999 0.599999) (drill 0.299999) (layers *.Cu *.Mask)
    (solder_paste_margin -49.999999) (zone_connect 2) (tstamp e8553ddc-d3a8-4764-9547-3ac2ed76484f))
  (pad "E4" thru_hole circle locked (at 17.9 -9.975 180) (size 0.599999 0.599999) (drill 0.299999) (layers *.Cu *.Mask)
    (solder_paste_margin -49.999999) (zone_connect 2) (tstamp 8a42b2f6-ddb3-4481-82d7-180454782e1e))
  (pad "G" smd rect (at 0.15 -10.1) (size 0.25 13.65) (layers "F.Cu")
    (zone_connect 2) (tstamp 0196d504-b4c5-4cce-9089-cfd25dba1295))
  (pad "G" smd rect (at 0.15 -10.1) (size 0.25 13.65) (layers "B.Cu")
    (zone_connect 2) (tstamp 17ca8cee-23ed-4a76-baa7-c005da1efb5c))
  (pad "G" smd rect (at 9.125 -16.8 90) (size 0.25 18.2) (layers "F.Cu")
    (zone_connect 2) (tstamp 1c296373-2a80-4f06-89c5-ce26d48660f8))
  (pad "G" smd rect (at 18.1 -13.7) (size 0.25 6.45) (layers "F.Cu")
    (zone_connect 2) (tstamp 34d9d2f7-268a-4994-8d5b-7a7defb4e42a))
  (pad "G" smd rect (at 9.125 -0.15 90) (size 0.25 18.2) (layers "B.Cu")
    (zone_connect 2) (tstamp 387509a2-a831-4566-a6ed-013a31ff81e0))
  (pad "G" smd rect (at 0.15 -0.65) (size 0.25 1.25) (layers "F.Cu")
    (zone_connect 2) (tstamp 427551ff-0943-4349-abe6-0de7da87ad35))
  (pad "G" smd rect (at 18.1 -0.2) (size 0.25 0.35) (layers "B.Cu")
    (zone_connect 2) (tstamp 73d13a59-4604-4348-afcc-2b0d9df35517))
  (pad "G" smd rect (at 18.1 -4.625) (size 0.25 6.5) (layers "F.Cu")
    (zone_connect 2) (tstamp beee0d02-ba47-4a0c-a558-f6c6f9fa9e4f))
  (pad "G" smd rect (at 18.1 -4.625) (size 0.25 6.5) (layers "B.Cu")
    (zone_connect 2) (tstamp befedf55-7739-41ca-9cf3-67cda2a1e135))
  (pad "G" smd rect (at 9.125 -0.15 90) (size 0.25 18.2) (layers "F.Cu")
    (zone_connect 2) (tstamp c86ff3cd-0649-48ad-9dd2-082e6511b4f0))
  (pad "G" smd rect (at 0.15 -0.65) (size 0.25 1.25) (layers "B.Cu")
    (zone_connect 2) (tstamp d57eaf46-3014-4866-ad5d-10af49f46492))
  (pad "G" smd rect (at 18.1 -0.2) (size 0.25 0.35) (layers "F.Cu")
    (zone_connect 2) (tstamp da1993a8-3ffb-4c80-bf92-1d10d0c3398e))
  (pad "G" smd rect (at 18.1 -13.7) (size 0.25 6.45) (layers "B.Cu")
    (zone_connect 2) (tstamp edd83707-12ab-4945-889e-3caa361baa52))
  (pad "G" smd rect (at 9.125 -16.8 90) (size 0.25 18.2) (layers "B.Cu")
    (zone_connect 2) (tstamp f7e4bace-825f-499c-8016-e2e07ff93d20))
  (pad "W1" thru_hole circle locked (at 0.375 -2.775 180) (size 0.599999 0.599999) (drill 0.299999) (layers *.Cu *.Mask)
    (solder_paste_margin -49.999999) (zone_connect 2) (tstamp 5ef4003d-d99e-480b-8c52-49fc5cb9ca06))
  (pad "W2" thru_hole circle locked (at 0.375 -1.775 180) (size 0.599999 0.599999) (drill 0.299999) (layers *.Cu *.Mask)
    (solder_paste_margin -49.999999) (zone_connect 2) (tstamp cca63b1a-8aa3-4325-ac24-e197aeea0971))
  (zone (net 0) (net_name "") (layers *.Cu) (tstamp 9ddcb69b-b5bb-488e-94da-4d62448828d1) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.025 -0.2)
        (xy 0.2 -0.225)
        (xy 0.175 -16.725)
        (xy 18.025 -16.725)
      )
    )
  )
)
