// this file was generated automatically by rusEfi tool ConfigDefinition.jar based on gen_config.sh integration/rusefi_config.txt Tue Nov 03 17:20:09 UTC 2020

// by class com.rusefi.output.FileFsioSettingsConsumer
	case FSIO_SETTING_FANONTEMPERATURE:
		return engineConfiguration->fanOnTemperature;
	case FSIO_SETTING_FANOFFTEMPERATURE:
		return engineConfiguration->fanOffTemperature;
	case FSIO_SETTING_ACIDLEEXTRAOFFSET:
		return engineConfiguration->acIdleExtraOffset;
	case FSIO_SETTING_ACIDLEEXTRAMIN:
		return engineConfiguration->acIdleExtraMin;
	case FSIO_SETTING_BOOSTPID_OFFSET:
		return engineConfiguration->boostPid.offset;
	case FSIO_SETTING_BOOSTPID_MINVALUE:
		return engineConfiguration->boostPid.minValue;
	case FSIO_SETTING_ALTERNATORCONTROL_OFFSET:
		return engineConfiguration->alternatorControl.offset;
	case FSIO_SETTING_ALTERNATORCONTROL_MINVALUE:
		return engineConfiguration->alternatorControl.minValue;
	case FSIO_SETTING_ETB_OFFSET:
		return engineConfiguration->etb.offset;
	case FSIO_SETTING_ETB_MINVALUE:
		return engineConfiguration->etb.minValue;
	case FSIO_SETTING_IDLERPMPID_OFFSET:
		return engineConfiguration->idleRpmPid.offset;
	case FSIO_SETTING_IDLERPMPID_MINVALUE:
		return engineConfiguration->idleRpmPid.minValue;
	case FSIO_SETTING_STARTUPFUELPUMPDURATION:
		return engineConfiguration->startUpFuelPumpDuration;
	case FSIO_SETTING_ETBWASTEGATEPID_OFFSET:
		return engineConfiguration->etbWastegatePid.offset;
	case FSIO_SETTING_ETBWASTEGATEPID_MINVALUE:
		return engineConfiguration->etbWastegatePid.minValue;
	case FSIO_SETTING_AUXPID1_OFFSET:
		return engineConfiguration->auxPid[0].offset;
	case FSIO_SETTING_AUXPID1_MINVALUE:
		return engineConfiguration->auxPid[0].minValue;
	case FSIO_SETTING_AUXPID2_OFFSET:
		return engineConfiguration->auxPid[1].offset;
	case FSIO_SETTING_AUXPID2_MINVALUE:
		return engineConfiguration->auxPid[1].minValue;
	case FSIO_SETTING_AUXPID3_OFFSET:
		return engineConfiguration->auxPid[2].offset;
	case FSIO_SETTING_AUXPID3_MINVALUE:
		return engineConfiguration->auxPid[2].minValue;
	case FSIO_SETTING_AUXPID4_OFFSET:
		return engineConfiguration->auxPid[3].offset;
	case FSIO_SETTING_AUXPID4_MINVALUE:
		return engineConfiguration->auxPid[3].minValue;
	case FSIO_SETTING_IDLETIMINGPID_OFFSET:
		return engineConfiguration->idleTimingPid.offset;
	case FSIO_SETTING_IDLETIMINGPID_MINVALUE:
		return engineConfiguration->idleTimingPid.minValue;
	case FSIO_SETTING_IDLERPMPID2_OFFSET:
		return engineConfiguration->idleRpmPid2.offset;
	case FSIO_SETTING_IDLERPMPID2_MINVALUE:
		return engineConfiguration->idleRpmPid2.minValue;
