CATEGORY=Parameters\Extras\Fuel Cut

PAGE_DESCRIPTION_START_HERE

IMG1=helpFuelCut.png

LABEL1=
Fuel Cut settings are conditions in which the engine will cut fuel on deceleration.

The Load setting is a basis. Depending on RPM it may cut slightly higher or lower
than the specified load.

Below Throttle Position. The vehicle must be below this throttle position to cut fuel.

Minimum RPM. The vehicle must be above this RPM to cut fuel.

Fuel cut delay is the amount of time before the fuel cut becomes active and
zeros out the fuel.
!LABEL1