P0001,Fuel Volume Regulator Control Circuit/Open
P0002,Fuel Volume Regulator Control Circuit Range/Performance
P0003,Fuel Volume Regulator Control Circuit Low
P0004,Fuel Volume Regulator Control Circuit High
P0005,Fuel Shutoff Valve Control Circuit/Open
P0006,Fuel Shutoff Valve Control Circuit Low
P0007,Fuel Shutoff Valve Control Circuit High
P0008,Engine Position System Performance (Bank1)
P0009,Engine Position System Performance (Bank2)
P0010,A Camshaft Position Actuator Circuit (Bank1)
P0011,A Camshaft Position - Timing Over-Advanced or System Performance (Bank 1)
P0012,A Camshaft Position - Timing Over-Retarded (Bank 1)
P0013,B Camshaft Position - Actuator Circuit (Bank1)
P0014,B Camshaft Position - Timing Over-Advanced or Sytem Performance (Bank 1)
P0015,B Camshaft Position - Timing Over-Retarded (Bank 1)
P0016,Crankshaft Position Camshaft Position Correlation (Bank 1 Sensor A)
P0017,Crankshaft Position Camshaft Position Correlation (Bank 1 Sensor B)
P0018,Crankshaft Position Camshaft Position Correlation (Bank 2 Sensor A)
P0019,Crankshaft Position Camshaft Position Correlation (Bank 2 Sensor B)
P0020,A Camshaft Position Actuator Circuit (Bank 2)
P0021,A Camshaft Position - Timing Over-Advanced or System Performance (Bank 2)
P0022,A Camshaft Position - Timing Over-Retarded (Bank 2)
P0023,B Camshaft Position - Actuator Circuit (Bank 2)
P0024,B Camshaft Position - Timing Over-Advanced or System Performance (Bank 2)
P0025,B Camshaft Position - Timing Over-Retarded (Bank 2)
P0026,Intake Valve Control Solenoid Circuit Range/Performance (Bank 1)
P0027,Exhaust Valve Control Solenoid Circuit Range/Performance (Bank 1)
P0028,Intake Valve Control Solenoid Circuit Range/Performance (Bank 2)
P0029,Exhaust Valve Control Solenoid Circuit Range/Performance (Bank 2)
P0030,HO2S Heater Control Circuit (Bank 1 Sensor 1)
P0031,HO2S Heater Control Circuit Low (Bank 1 Sensor 1)
P0032,HO2S Heater Control Circuit High (Bank 1 Sensor 1)
P0033,Turbo Charger Bypass Valve Control Circuit
P0034,Turbo Charger Bypass Valve Control Circuit Low
P0035,Turbo Charger Bypass Valve Control Circuit High
P0036,HO2S Heater Control C ircuit (Bank 1 Sensor 2)
P0037,HO2S Heater Control Circuit Low (Bank 1 Sensor 2)
P0038,HO2S Heater Control Circuit High (Bank 1 Sensor 2)
P0039,Turbo/Super Charger Bypass Valve Control Circuit Range/Performance
P0040,O2 Sensor Signals Swapped Bank 1 Sensor 1/ Bank 2 Sensor 1
P0041,O2 Sensor Signals Swapped Bank 1 Sensor 2/ Bank 2 Sensor 2
P0042,HO2S Heater Control Circuit (Bank 1 Sensor 3)
P0043,HO2S Heater Control Circuit Low (Bank 1 Sensor 3)
P0044,HO2S Heater Control Circuit High (Bank 1 Sensor 3)
P0045,Turbo/Super Charger Boost Control Solenoid Circuit/Open
P0046,Turbo/Super Charger Boost Control Solenoid Circuit Range/Performance
P0047,Turbo/Super Charger Boost Control Solenoid Circuit Low
P0048,Turbo/Super Charger Boost Control Solenoid Circuit High
P0049,Turbo/Super Charger Turbine Overspeed
P0050,HO2S Heater Control Circuit (Bank 2 Sensor 1)
P0051,HO2S Heater Control Circuit Low (Bank 2 Sensor 1)
P0052,HO2S Heater Control Circuit High (Bank 2 Sensor 1)
P0053,HO2S Heater Resistance (Bank 1 Sensor 1)
P0054,HO2S Heater Resistance (Bank 1 Sensor 2)
P0055,HO2S Heater Resistance (Bank 1 Sensor 3)
P0056,HO2S Heater Control Circuit (Bank 2 Sensor 2)
P0057,HO2S Heater Control Circuit Low (Bank 2 Sensor 2)
P0058,HO2S Heater Control Circuit High (Bank 2 Sensor 2)
P0059,HO2S Heater Resistance (Bank 2 Sensor 1)
P0060,HO2S Heater Resistance (Bank 2 Sensor 2)
P0061,HO2S Heater Resistance (Bank 2 Sensor 3)
P0062,HO2S Heater Control Circuit (Bank 2 Sensor 3)
P0063,HO2S Heater Control Circuit Low (Bank 2 Sensor 3)
P0064,HO2S Heater Control Circuit High (Bank 2 Sensor 3)
P0065,Air Assisted Injector Control Range/Performance
P0066,Air Assisted Injector Control Circuit or Circuit Low
P0067,Air Assisted Injector Control Circuit High
P0068,MAP/MAF Throttle Position Correlation
P0069,Manifold Absolute Pressure Barometric Pressure Correlation
P0070,Ambient Air Temperature Sensor Circuit
P0071,Ambient Air Temperature Sensor Range/Performance
P0072,Ambient Air Temperature Sensor Circuit Low
P0073,Ambient Air Temperature Sensor Circuit High
P0074,Ambient Air Temperature Sensor Circuit Intermittent
P0075,Intake Valve Control Solenoid Circuit (Bank 1)
P0076,Intake Valve Control Solenoid Circuit Low (Bank 1)
P0077,Intake Valve Control Solenoid Circuit High (Bank 1)
P0078,Exhaust Valve Control Solenoid Circuit (Bank 1)
P0079,Exhaust Valve Control Solenoid Circuit Low (Bank 1)
P0080,Exhaust Valve Control Solenoid C ircuit High (Bank 1)
P0081,Intake Valve Control Solenoid Circuit (Bank 2)
P0082,Intake Valve Control Solenoid Circuit Low (Bank 2)
P0083,Intake Valve Control Solenoid Circuit High (Bank 2)
P0084,Exhaust Valve Control Solenoid Circuit (Bank 2)
P0085,Exhaust Valve Control Solenoid Circuit Low (Bank 2)
P0086,Exhaust Valve Control Solenoid C ircuit High (Bank 2)
P0087,Fuel Rail/System Pressure - Too Low
P0088,Fuel Rail/System Pressure - Too High
P0089,Fuel Pressure Regulator 1 Performance
P0090,Fuel Pressure Regulator 1 Control Circuit
P0091,Fuel Pressure Regulator 1 Control Circuit Low
P0092,Fuel Pressure Regulator 1 Control Circuit High
P0093,Fuel System Leak Detected Large Leak
P0094,Fuel System Leak Detected Small Leak
P0095,Intake Air Temperature Sensor 2 Circuit
P0096,Intake Air Temperature Sensor 2 Circuit Range/Performance
P0097,Intake Air Temperature Sensor 2 Circuit Low
P0098,Intake Air Temperature Sensor 2 Circuit High
P0099,Intake Air Temperature Sensor 2 Circuit Intermittent/Erratic
P0100,Mass or Volume Air flow Circuit Malfunction
P0101,Mass or Volume Air flow Circuit Range/Performance Problem
P0102,Mass or Volume Air Flow Circuit low Input
P0103,Mass or Volume Air flow Circuit High Input
P0104,Mass or Volume Air flow Circuit Intermittent
P0105,Manifold Absolute Pressure/Barometric Pressure Circuit Malfunction
P0106,Manifold Absolute Pressure/Barometric Pressure Circuit Range/Performance Problem
P0107,Manifold Absolute Pressure/Barometric Pressure Circuit Low Input
P0108,Manifold Absolute Pressure/Barometric Pressure Circuit High Input
P0109,Manifold Absolute Pressure/Barometric Pressure Circuit Intermittent
P0110,Intake Air Temperature Circuit Malfunction
P0111,Intake Air Temperature Circuit Range/Performance Problem
P0112,Intake Air Temperature Circuit Low Input
P0113,Intake Air Temperature Circuit High Input
P0114,Intake Air Temperature Circuit Intermittent
P0115,Engine Coolant Temperature Circuit Malfunction
P0116,Engine Coolant Temperature Circuit Range/Performance Problem
P0117,Engine Coolant Temperature Circuit Low Input
P0118,Engine Coolant Temperature Circuit High Input
P0119,Engine Coolant Temperature Circuit Intermittent
P0120,Throttle Pedal Position Sensor/Switch A Circuit Malfunction
P0121,Throttle/Pedal Position Sensor/Switch A Circuit Range/Performance Problem
P0122,Throttle/Pedal Position Sensor/Switch A Circuit Low Input
P0123,Throttle/Pedal Position Sensor/Switch A Circuit High Input
P0124,Throttle/Pedal Position Sensor/Switch A Circuit Intermittent
P0125,Insufficient Coolant Temperature for Closed Loop Fuel Control
P0126,Insufficient Coolant Temperature for Stable Operation
P0130,O2 Sensor Circuit Malfunction (Bank 1 Sensor 1)
P0131,O2 Sensor Circuit Low Voltage (Bank 1 Sensor 1)
P0132,O2 Sensor Circuit High Voltage (Bank 1 Sensor 1)
P0133,O2 Sensor Circuit Slow Response (Bank 1 Sensor 1)
P0134,O2 Sensor Circuit No Activity Detected (Bank 1 Sensor 1)
P0135,O2 Sensor Heater Circuit Malfunction (Bank 1 Sensor 1)
P0136,O2 Sensor Circuit Malfunction (Bank 1 Sensor 2)
P0137,O2 Sensor Circuit Low Voltage (Bank 1 Sensor 2)
P0138,O2 Sensor Circuit High Voltage (Bank 1 Sensor 2)
P0139,O2 Sensor Circuit Slow Response (Bank 1 Sensor 2)
P0140,O2 Sensor Circuit No Activity Detected (Bank 1 Sensor 2)
P0141,O2 Sensor Heater Circuit Malfunction (Bank 1 Sensor 2)
P0142,O2 Sensor Circuit Malfunction (Bank 1 Sensor 3)
P0143,O2 Sensor Circuit Low Voltage (Bank 1 Sensor 3)
P0144,O2 Sensor Circuit High Voltage (Bank 1 Sensor 3)
P0145,O2 Sensor Circuit Slow Response (Bank 1 Sensor 3)
P0146,O2 Sensor Circuit No Activity Detected (Bank 1 Sensor 3
P0147,O2 Sensor Heater Circuit Malfunction (Bank 1 Sensor 3)
P0150,O2 Sensor Circuit Malfunction (Bank 2 Sensor 1)
P0151,O2 Sensor Circuit Low Voltage (Bank 2 Sensor 1)
P0152,O2 Sensor Circuit High Voltage (Bank 2 Sensor 1)
P0153,O2 Sensor Circuit Slow Response (Bank 2 Sensor 1)
P0154,O2 Sensor Circuit No Activity Detected (Bank 2 Sensor 1)
P0155,O2 Sensor Heater Circuit Malfunction (Bank 2 Sensor 1
P0156,O2 Sensor Circuit Malfunction (Bank 2 Sensor 2)
P0157,O2 Sensor Circuit Low Voltage (Bank 2 Sensor 2)
P0158,O2 Sensor Circuit High Voltage (Bank 2 Sensor 2)
P0159,O2 Sensor Circuit Slow Response (Bank 2 Sensor 2
P0160,O2 Sensor Circuit No Activity Detected (Bank 2 Sensor 2)
P0161,O2 Sensor Heater Circuit Malfunction (Bank 2 Sensor 2)
P0162,O2 Sensor Circuit Malfunction (Bank 2 Sensor 3
P0163,O2 Sensor Circuit Low Voltage (Bank 2 Sensor 3
P0164,O2 Sensor Circuit High Voltage (Bank 2 Sensor 3)
P0165,O2 Sensor Circuit Slow Response (Bank 2 Sensor 3)
P0166,O2 Sensor Circuit No Activity Detected (Bank 2 Sensor 3
P0167,O2 Sensor Heater Circuit Malfunction (Bank 2 Sensor 3)
P0170,Fuel Trim Malfunction (Bank 1)
P0171,System Too Lean (Bank 1)
P0172,System Too Rich (Bank 1)
P0173,Fuel Trim Malfunction (Bank 2)
P0174,System Too Lean (Bank 2
P0175,System Too Rich (Bank 2)
P0176,Fuel Composition Sensor Circuit Malfunction
P0177,Fuel Composition Sensor Circuit Range/Performance
P0178,Fuel Composition Sensor Circuit Low Input
P0179,Fuel Composition Sensor Circuit High Input
P0180,Fuel Temperature Sensor A Circuit Malfunction
P0181,Fuel Temperature Sensor A Circuit Performance
P0182,Fuel Temperature Sensor A Circuit low Input
P0183,Fuel Temperature Sensor A Circuit High Input
P0184,Fuel Temperature Sensor A Circuit Intermittent
P0185,Fuel Temperature Sensor B Circuit Malfunction
P0186,Fuel Temperature Sensor B Circuit Range/Performance
P0187,Fuel Temperature Sensor U Circuit Low Input
P0188,Fuel Temperature Sensor B Circuit High Input
P0189,Fuel Temperature Sensor B Circuit Intermittent
P0190,Fuel Rail Pressure Sensor Circuit Malfunction
P0191,Fuel Rail Pressure Sensor Circuit Range/Performance
P0192,Fuel Rail Pressure Sensor Circuit Low Input
P0193,Fuel Rail Pressure Sensor Circuit High Input
P0194,Fuel Rail Pressure Sensor Circuit Intermittent
P0195,Engine Oil Temperature Sensor Malfunction
P0196,Engine Oil Temperature Sensor Range/Performance
P0197,Engine Oil Temperature Sensor Low
P0198,Engine Oil Temperature Sensor High
P0199,Engine Oil Temperature Sensor Intermittent
P0200,Injector Circuit Malfunction
P0201,Injector Circuit Malfunction - Cylinder 1
P0202,Injector Circuit Malfunction - Cylinder 2
P0203,Injector Circuit Malfunction - Cylinder 3
P0204,Injector Circuit Malfunction - Cylinder 4
P0205,Injector Circuit Malfunction - Cylinder 5
P0206,Injector Circuit Malfunction - Cylinder 6
P0207,Injector Circuit Malfunction - Cylinder 7
P0208,Injector Circuit Malfunction - Cylinder 8
P0209,Injector Circuit Malfunction - Cylinder 9
P0210,Injector Circuit Malfunction - Cylinder 10
P0211,Injector Circuit Malfunction - Cylinder 11
P0212,Injector Circuit Malfunction - Cylinder 12
P0213,Cold Start Injector 1 Malfunction
P0214,Cold Start Injector 2 Malfunction
P0215,Engine Shutoff Solenoid Malfunction
P0216,Injection Timing Control Circuit Malfunction
P0217,Engine Overtemp Condition
P0218,Transmission Over Temperature Condition
P0219,Engine Over Speed Condition
P0220,Throttle/Pedal Position Sensor/Switch B Circuit Malfunction
P0221,Throttle/pedal Position Sensor/Switch B Circuit Range/Performance Problem
P0222,Throttle/pedal Position Sensor/Switch B Circuit Low Input
P0223,Throttle/Pedal Position Sensor/Switch B Circuit High Input
P0224,Throttle/Pedal Position Sensor/Switch B Circuit Intermittent
P0225,Throttle/Pedal Position Sensor/Switch C Circuit Malfunction
P0226,Throttle/Pedal Position Sensor/Switch C Circuit Range/Performance Problem
P0227,Throttle/Pedal Position Sensor/Switch C Circuit Low Input
P0228,Throttle/Pedal Position Sensor/Switch C Circuit High Input
P0229,Throttle/Pedal Position Sensor/Switch C Circuit Intermittent
P0230,Fuel Pump Primary Circuit Malfunction
P0231,Fuel Pump Secondary Circuit Low
P0232,Fuel Pump Secondary Circuit High
P0233,Fuel Pump Secondary Circuit Intermittent
P0234,Engine Overboost Condition
P0235,Turbocharger Boost Sensor A Circuit Malfunction
P0236,Turbocharger Boost Sensor A Circuit Range/Performance
P0237,Turbocharger Boost Sensor A Circuit Low
P0238,Turbocharger Boost Sensor A Circuit High
P0239,Turbocharger Boost Sensor B Circuit Malfunction
P0240,Turbocharger Boost Sensor B Circuit Range/Performance
P0241,Turbocharger Boost Sensor B Circuit Low
P0242,Turbocharger Boost Sensor B Circuit High
P0243,Turbocharger Wastegate Solenoid A Malfunction
P0244,Turbocharger Wastegate Solenoid A Range/Performance
P0245,Turbocharger Wastegate Solenoid A low
P0246,Turbocharger Wastegate Solenoid A High
P0247,Turbocharger Wastegate Solenoid B Malfunction
P0248,Turbocharger Wastegate Solenoid B Range/Performance
P0249,Turbocharger Wastegate Solenoid B Low
P0250,Turbocharger Wastegate Solenoid B High
P0251,Injection Pump Fuel Metering Control 'A' Malfunction (Cam/Rotor/Injector)
P0252,Injection Pump Fuel Metering Control 'A' Range/Performance (Cam/Rotor/Injector)
P0254,Injection Pump Fuel Metering Control 'A' High (Cam/Rotor/Injector)
P0256,Injection Pump Fuel Metering Control 'B' Malfunction (Cam/Rotor/Injector)
P0257,Injection Pump Fuel Metering Control 'B' Range/Performance (Cam/Rotor/Injector)
P0258,Injection Pump Fuel Metering Control 'B' Low (Cam/Rotor/Injector)
P0259,Injection lump Fuel Metering Control 'B' High (Cam/Rotor/Injector)
P0260,Injection Pump Fuel Metering Control 'B' Intermittent (Cam/Rotor/Injector)
P0261,Cylinder 1 Injector Circuit Low
P0262,Cylinder 1 Injector Circuit High
P0263,Cylinder 1 Contribution/Balance Fault
P0264,Cylinder 2 Injector Circuit Low
P0265,Cylinder 2 Injector Circuit High
P0266,Cylinder 2 Contribution/Balance Fault
P0267,Cylinder 3 Injector Circuit Low
P0268,Cylinder 3 Injector Circuit High
P0269,Cylinder 3 Contribution/Balance Fault
P0270,Cylinder 4 Injector Circuit Low
P0271,Cylinder 4 Injector Circuit High
P0272,Cylinder 4 Contribution/Balance Fault
P0273,Cylinder 5 Injector Circuit Low
P0274,Cylinder 5 Injector Circuit High
P0275,Cylinder 5 Contribution/Balance Fault
P0276,Cylinder 6 Injector Circuit Low
P0277,Cylinder 6 Injector Circuit High
P0278,Cylinder 6 Contribution/Balance Fault
P0279,Cylinder 7 Injector Circuit Low
P0280,Cylinder 7 Injector Circuit High
P0281,Cylinder 7 Contribution/Balance Fault
P0282,Cylinder 8 Injector Circuit Low
P0283,Cylinder 8 Injector Circuit High
P0284,Cylinder 8 Contribution/Balance Fault
P0285,Cylinder 9 Injector Circuit Low
P0286,Cylinder 9 Injector Circuit High
P0287,Cylinder 9 Contribution/Balance Fault
P0288,Cylinder 10 Injector Circuit Low
P0289,Cylinder 10 Injector Circuit High
P0290,Cylinder 10 Contribution/balance Fault
P0291,Cylinder 11 Injector Circuit Low
P0292,Cylinder 11 Injector Circuit High
P0293,Cylinder 11 Contribution/balance Fault
P0294,Cylinder 12 Injector Circuit Low
P0295,Cylinder 12 Injector Circuit High
P0296,Cylinder 12 Contribution/Balance Fault
P0300,Random/Multiple Cylinder Misfire Detected
P0301,Cylinder 1 Misfire Detected
P0302,Cylinder 2 Misfire Detected
P0303,Cylinder 3 Misfire Detected
P0304,Cylinder 4 Misfire Detected
P0305,Cylinder 5 Misfire Detected
P0306,Cylinder 6 Misfire Detected
P0307,Cylinder 7 Misfire Detected
P0308,Cylinder 8 Misfire Detected
P0309,Cylinder 9 Misfire Detected
P0310,Cylinder 10 Misfire Detected
P0311,Cylinder 11 Misfire Detected
P0312,Cylinder 12 Misfire Detected
P0320,Ignition/Distributor Engine Speed Input Circuit Malfunction
P0321,Ignition/Distributor Engine Speed Input Circuit Range/Performance
P0322,Ignition/Distributor Engine Speed Input Circuit No Signal
P0323,Ignition/Distributor Engine Speed Input Circuit Intermittent
P0325,Knock Sensor 1 Circuit Malfunction (Bank 1 or Single Sensor
P0326,Knock Sensor 1 Circuit Range/Performance (Bank 1 or Single Sensor)
P0327,Knock Sensor 1 Circuit low Input (Bank 1 or Single Sensor)
P0328,Knock Sensor 1 Circuit High Input (Bank 1 or Single Sensor)
P0329,Knock Sensor 1 Circuit Input Intermittent (Bank 1 or Single Sensor)
P0330,Knock Sensor 2 Circuit Malfunction (Bank 2)
P0331,Knock Sensor 2 Circuit Range/Performance (Bank 2)
P0332,Knock Sensor 2 Circuit Low Input (Bank 2)
P0333,Knock Sensor 2 Circuit High Input (Bank 2)
P0334,Knock Sensor 2 Circuit Input Intermittent (Bank 2)
P0335,Crankshaft Position Sensor A Circuit Malfunction
P0336,Crankshaft Position Sensor A Circuit Range/Performance
P0337,Crankshaft Position Sensor A Circuit Low Input
P0338,Crankshaft Position Sensor A Circuit High Input
P0339,Crankshaft Position Sensor A Circuit Intermittent
P0340,Camshaft Position Sensor Circuit Malfunction
P0341,Camshaft Position Sensor Circuit Range/Performance
P0342,Camshaft Position Sensor Circuit Low Input
P0343,Camshaft Position Sensor Circuit High Input
P0344,Camshaft Position Sensor Circuit Intermittent
P0350,Ignition Coil Primary/Secondary Circuit Malfunction
P0351,Ignition Coil A Primary/Secondary Circuit Malfunction
P0352,Ignition Coil B Primary/Secondary Circuit Malfunction
P0353,Ignition Coil C Primary/Secondary Circuit Malfunction
P0354,Ignition Coil D Primary/Secondary Circuit Malfunction
P0355,Ignition Coil B Primary/Secondary Circuit Malfunction
P0356,Ignition Coil F Primary/Secondary Circuit Malfunction
P0357,Ignition Coil G Primary/Secondary Circuit Malfunction
P0358,Ignition Coil H Primary/Secondary Circuit Malfunction
P0359,Ignition Coil I Primary/Secondary Circuit Malfunction
P0360,Ignition Coil I Primary/Secondary Circuit Malfunction
P0361,Ignition Coil K Primary/Secondary Circuit Malfunction
P0362,Ignition Coil L Primary/Secondary Circuit Malfunction
P0370,Timing Reference High Resolution Signal A Malfunction
P0371,Timing Reference High Resolution Signal A Too Many Pulses
P0372,Timing Reference High Resolution Signal A Too Few Pulses
P0373,Timing Reference High Resolution Signal A Intermittent/Erratic Pulses
P0374,Timing Reference High Resolution Signal A No Pulses
P0375,Timing Reference High Resolution Signal B Malfunction
P0376,Timing Reference High Resolution Signal B Too Many Pulses
P0377,Timing Reference High Resolution Signal B Too Few Pulses
P0378,Timing Reference High Resolution Signal B Intermittent/Erratic Pulses
P0379,Timing Reference High Resolution Signal B No Pulses
P0380,Glow Plug/Heater Circuit 'A' Malfunction
P0381,Glow Plug/Heater Indicator Circuit Malfunction
P0382,Glow Plug/Heater Circuit 'B' Malfunction
P0385,Crankshaft Position Sensor B Circuit Malfunction
P0386,Crankshaft Position Sensor B Circuit Range/Performance
P0387,Crankshaft Position Sensor B Circuit Low Input
P0388,Crankshaft Position Sensor B Circuit High Input
P0389,Crankshaft Position Sensor B Circuit Intermittent
P0400,Exhaust Gas Recirculation Flow Malfunction
P0401,Exhaust Gas Recirculation Flow Insufficient Detected
P0402,Exhaust Gas Recirculation Flow Excessive Detected
P0403,Exhaust Gas Recirculation Circuit Malfunction
P0404,Exhaust Gas Recirculation Circuit Range/Performance
P0405,Exhaust Gas Recirculation Sensor A Circuit Low
P0406,Exhaust Gas Recirculation Sensor A Circuit High
P0407,Exhaust Gas Recirculation Sensor B Circuit Low
P0408,Exhaust Gas Recirculation Sensor B Circuit High
P0410,Secondary Air Injection System Malfunction
P0411,Secondary Air Injection System Incorrect Flow Detected
P0412,Secondary Air Injection System Switching Valve A Circuit Malfunction
P0413,Secondary Air Injection System Switching Valve A Circuit Open
P0414,Secondary Air Injection System Switching Valve A Circuit Shorted
P0415,Secondary Air Injection System Switching Valve B Circuit Malfunction
P0416,Secondary Air Injection System Switching Valve B Circuit Open
P0417,Secondary Air Injection System Switching Valve B Circuit Shorted
P0418,Secondary Air Injection System Relay A circuit Malfunction
P0419,Secondary Air Injection System Relay B Circuit Malfunction
P0420,Catalyst System Efficiency Below Threshold (Bank 1)
P0421,Warm Up Catalyst Efficiency Below Threshold (Bank 1
P0422,Main Catalyst Efficiency Below Threshold (Bank 1
P0423,Heated Catalyst Efficiency Below Threshold (Bank l)
P0424,Heated Catalyst Temperature Below Threshold (Bank 1)
P0430,Catalyst System Efficiency Below Threshold (Bank 2)
P0431,Warm Up Catalyst Efficiency Below Threshold (Bank 2)
P0432,Main Catalyst Efficiency Below Threshold (Bank 2)
P0433,Heated Catalyst Efficiency Below Threshold (Bank 2)
P0434,Heated Catalyst Temperature Below Threshold (Bank 2)
P0440,Evaporative Emission Control System Malfunction
P0441,Evaporative Emission Control System Incorrect Purge flow
P0442,Evaporative Emission Control System leak Detected (small leak)
P0443,Evaporative Emission Control System Purge Control Valve circuit Malfunction
P0444,Evaporative Emission Control System Purge Control Valve Circuit Open
P0445,Evaporative Emission Control System Purge Control Valve Circuit Shorted
P0446,Evaporative Emission Control System Vent Control Circuit Malfunction
P0447,Evaporative Emission Control System Vent Control Circuit Open
P0448,Evaporative Emission Control System Vent Control Circuit Shorted
P0449,Evaporative Emission Control System Vent Valve/Solenoid Circuit Malfunction
P0450,Evaporative Emission Control System Pressure Sensor Malfunction
P0451,Evaporative Emission Control System Pressure Sensor Range/Performance
P0452,Evaporative Emission Control System Pressure Sensor Low Input
P0453,Evaporative Emission Control System Pressure Sensor High Input
P0454,Evaporative Emission Control System Pressure Sensor Intermittent
P0455,Evaporative Emission Control System Tank Detected (gross leak)
P0460,Fuel Level Sensor Circuit Malfunction
P0461,Fuel Level Sensor Circuit Range/Performance
P0462,Fuel level Sensor Circuit Low Input
P0463,Fuel level Sensor Circuit High Input
P0464,Fuel level Sensor Circuit Intermittent
P0465,Purge Flow Sensor Circuit Malfunction
P0466,Purge flow Sensor Circuit Range/Performance
P0467,Purge Flow Sensor Circuit Low Input
P0468,Purge flow Sensor Circuit High Input
P0469,Purge flow Sensor Circuit Intermittent
P0470,Exhaust Pressure Sensor Malfunction
P0471,Exhaust Pressure Sensor Range/Performance
P0472,Exhaust Pressure Sensor Low
P0473,Exhaust Pressure Sensor High
P0474,Exhaust Pressure Sensor Intermittent
P0475,Exhaust Pressure Control Valve Malfunction
P0476,Exhaust Pressure Control Valve Range/Performance
P0477,Exhaust Pressure Control Valve Low
P0478,Exhaust Pressure Control Valve High
P0479,Exhaust Pressure Control Valve Intermittent
P0480,Cooling Fan 1 Control Circuit Malfunction
P0481,Cooling Fan 2 Control Circuit Malfunction
P0482,Cooling Fan 3 Control Circuit Malfunction
P0483,Cooling Fan Rationality Check Malfunction
P0484,Cooling Fan Circuit Over Current
P0485,Cooling Fan Power/Ground Circuit Malfunction
P0500,Vehicle Speed Sensor Malfunction
P0501,Vehicle Speed Sensor Range/Performance
P0502,Vehicle Speed Sensor Circuit Low Input
P0503,Vehicle Speed Sensor Intermittent/Erratic/High
P0505,Idle Control System Malfunction
P0506,Idle Control System RPM lower Than Expected
P0507,Idle Control System RPM higher Than Expected
P0510,Closed Throttle Position Switch Malfunction
P0520,Engine Oil Pressure Sensor/Switch Circuit Malfunction
P0521,Engine Oil Pressure Sensor/Switch Range/Performance
P0522,Engine Oil Pressure Sensor/Switch Low Voltage
P0523,Engine Oil Pressure Sensor/Switch High Voltage
P0530,A/C Refrigerant Pressure Sensor Circuit Malfunction
P0531,A/C Refrigerant Pressure Sensor Circuit Range/Performance
P0532,A/C Refrigerant Pressure Sensor Circuit Low Input
P0533,A/C Refrigerant pressure Sensor Circuit High Input
P0534,Air Conditioner Refrigerant Charge Loss
P0550,Power Steering Pressure Sensor Circuit Malfunction
P0551,Power Steering Pressure Sensor Circuit Range/Performance
P0552,Power Steering Pressure Sensor Circuit Low Input
P0553,Power Steering Pressure Sensor Circuit High Input
P0554,Power Steering Pressure sensor Circuit Intermittent
P0560,System Voltage Malfunction
P0561,System Voltage Unstable
P0562,System Voltage Low
P0563,System Voltage High
P0565,Cruise Control On Signal Malfunction
P0566,Cruise Control Off Signal Malfunction
P0567,Cruise Control Resume Signal Malfunction
P0568,Cruise Control Set Signal Malfunction
P0569,Cruise Control Coast Signal Malfunction
P0570,Cruise Control Accel Signal Malfunction
P0571,Cruise Control/Brake Switch A Circuit Malfunction
P0572,Cruise Control/Brake Switch A Circuit Low
P0573,Cruise Control/Brake Switch A Circuit High
P0574,through P0580 Reserved for Cruise Codes
P0600,Serial Communication Link Malfunction
P0601,Internal Control Module Memory Check Sum Error
P0602,Control Module Programming Error
P0603,Internal Control Module Keep Alive Memory (KAM) Error
P0604,Internal Control Module RAM Error
P0605,Internal Control Module ROM Error (Module Identification Defined by SAE J1979)
P0606,PCM Processor Fault
P0608,Control Module VSS Output 'A' Malfunction
P0609,Control Module VSS Output 'B' Malfunction
P0620,Generator Control Circuit Malfunction
P0621,Generator Lamp 'L' Control Circuit Malfunction
P0622,Generator Field 'F' Control Circuit Malfunction
P0650,Malfunction Indicator Lamp (MIL) Control Circuit Malfunction
P0654,Engine RPM Output Circuit Malfunction
P0655,Engine Hot Lamp Output Control Circuit Malfunction
P0656,Fuel Level Output Circuit Malfunction
P0700,Transmission Control System Malfunction
P0701,Transmission Control System Range/Performance
P0702,Transmission Control System Electrical
P0703,Torque Converter/Brake Switch B Circuit Malfunction
P0704,Clutch Switch Input Circuit Malfunction
P0705,Transmission Range Sensor Circuit malfunction (PRNDL Input)
P0706,Transmission Range Sensor Circuit Range/Performance
P0707,Transmission Range Sensor Circuit Low Input
P0708,Transmission Range Sensor Circuit High Input
P0709,Transmission Range Sensor Circuit Intermittent
P0710,Transmission Fluid Temperature Sensor Circuit Malfunction
P0711,Transmission Fluid Temperature Sensor Circuit Range/Performance
P0712,Transmission Fluid Temperature Sensor Circuit Low Input
P0713,Transmission Fluid Temperature Sensor Circuit High Input
P0714,Transmission Fluid Temperature Sensor Circuit Intermittent
P0715,Input/Turbine Speed Sensor Circuit Malfunction
P0716,Input/Turbine Speed Sensor Circuit Range/Performance
P0717,Input/Turbine Speed Sensor Circuit No Signal
P0718,Input/Turbine Speed Sensor Circuit Intermittent
P0719,Torque Converter/Brake Switch B Circuit Low
P0720,Output Speed Sensor Circuit Malfunction
P0721,Output Speed Sensor Range/Performance
P0722,Output Speed Sensor No Signal
P0723,Output Speed Sensor Intermittent
P0724,Torque Converter/Brake Switch B Circuit High
P0725,Engine Speed input Circuit Malfunction
P0726,Engine Speed Input Circuit Range/Performance
P0727,Engine Speed Input Circuit No Signal
P0728,Engine Speed Input Circuit Intermittent
P0730,Incorrect Gear Ratio
P0731,Gear 1 Incorrect ratio
P0732,Gear 2 Incorrect ratio
P0733,Gear 3 Incorrect ratio
P0734,Gear 4 Incorrect ratio
P0735,Gear 5 Incorrect ratio
P0736,Reverse incorrect gear ratio
P0740,Torque Converter Clutch Circuit Malfuction
P0741,Torque Converter Clutch Circuit Performance or Stuck Off
P0742,Torque Converter Clutch Circuit Stuck On
P0743,Torque Converter Clutch Circuit Electrical
P0744,Torque Converter Clutch Circuit Intermittent
P0745,Pressure Control Solenoid Malfunction
P0746,Pressure Control Solenoid Performance or Stuck Off
P0747,Pressure Control Solenoid Stuck On
P0748,Pressure Control Solenoid Electrical
P0749,Pressure Control Solenoid Intermittent
P0750,Shift Solenoid A Malfunction
P0751,Shift Solenoid A Performance or Stuck Off/1-2 Shift Solenoid Valve Performance
P0752,Shift Solenoid A Stuck On
P0753,Shift Solenoid A Electrical/1-2 Shift Solenoid Circuit Electrical
P0754,Shift Solenoid A Intermittent
P0755,Shift Solenoid B Malfunction
P0756,Shift Solenoid B Performance or Stuck Off/2-3 Shift Solenoid Valve Performance
P0757,Shift Solenoid B Stuck On
P0758,Shift Solenoid B Electrical/2-3 Shift Solenoid Circuit Electrical
P0759,Shift Solenoid B Intermittent
P0760,Shift Solenoid C Malfunction
P0761,Shift Solenoid C Performance or Stuck Off
P0762,Shift Solenoid C Stuck On
P0763,Shift Solenoid C Electrical
P0764,Shift Solenoid C Intermittent
P0765,Shift Solenoid D Malfunction
P0766,Shift Solenoid D Performance or Stuck Off
P0767,Shift Solenoid D Stuck On
P0768,Shift Solenoid D Electrical
P0769,Shift Solenoid D Intermittent
P0770,Shift Solenoid E Malfunction
P0771,Shift Solenoid E Performance or Stuck Off
P0772,Shift Solenoid E Stuck On
P0773,Shift Solenoid E Electrical
P0774,Shift Solenoid E Intermittent
P0775,Pressure Control Solenoid B Malfunction
P0776,Pressure Control Solenoid B Performance
P0777,Pressure Control Solenoid B Stuck On
P0778,Pressure Control Solenoid B Electrical
P0779,Pressure Control Solenoid B Intermittent
P0780,Shift Malfunction
P0781,1-2 Shift Malfunction
P0782,2-3 Shift Malfunction
P0783,3-4 Shift Malfunction
P0784,4-5 Shift Malfunction
P0785,Shift/Timing Solenoid Malfunction/ 3-2 Shift Solenoid Circuit Electrical
P0786,Shift/Timing Solenoid Range/Performance
P0787,Shift/Timing Solenoid Low
P0788,Shift/Timing Solenoid High
P0789,Shift/Timing Solenoid Intermittent
P0790,Normal/Performance Switch Circuit Malfunction
P0791,Intermediate Shaft Speed Sensor Circuit
P0792,Intermediate Shaft Speed Sensor Circuit Range/Performance
P0793,Intermediate Shaft Speed Sensor Circuit No signal
P0794,Intermediate Shaft Speed Sensor Circuit Intermittent
P0795,Pressure Control Solenoid C
P0796,Pressure Control Solenoid C Performance or Stuck off
P0797,Pressure Control Solenoid C Stuck On
P0798,Pressure Control Solenoid C Electrical
P0799,Pressure Control Solenoid C Intermittent
P0801,Reverse Inhibit Control Circuit Malfunction
P0803,1-4 Upshift (Skip Shift) Solenoid Control Circuit Malfunction
P0804,1-4 Upshift (Skip Shift) Lamp Control Circuit Malfunction
P0805,Clutch Position Sensor Circuit Malfunction
P0806,Clutch Position Sensor Circuit Range/Performance Malfunction
P0807,Clutch Position Sensor Circuit Low Malfunction
P0808,Clutch Position Sensor Circuit High Malfunction
P0809,Clutch Position Sensor Circuit Intermittent Malfunction
P0810,Clutch Position Control Error
P0811,Excessive Clutch Slippage
P0812,Reverse Input Circuit
P0813,Reverse Output Circuit
P0814,Transmission Range Display Circuit
P0815,Upshift Switch Circuit
P0816,Downshift Switch Circuit
P0817,Starter Disable Circuit
P0818,Driveline Disconnect Switch Input Circuit
P0819,Up and Down Shift Switch to Transmission Range Correlation
P0820,Gear Lever X - Y Position Sensor Circuit
P0821,Gear Lever X Position Circuit
P0822,Gear Lever Y Position Circuit
P0823,Gear Lever X Position Circuit Intermittent
P0824,Gear Lever Y Position Circuit Intermittent
P0825,Gear Lever Push - Pull Switch (Shift Anticipate)
P0826,Up and Down Switch Input Circuit
P0827,Up and Down Switch Input Circuit Low
P0828,Up and Down Switch Input Circuit High
P0829,5-6 Shift
P0830,Clutch Pedal Switch A Circuit
P0831,Clutch Pedal Switch A Circuit Low
P0832,Clutch Pedal Switch A Circuit High
P0833,Clutch Pedal Switch B Circuit
P0834,Clutch Pedal Switch B Circuit Low
P0835,Clutch Pedal Switch B Circuit High
P0836,Four Wheel Drive (4WD) Switch Circuit
P0837,Four Wheel Drive (4WD) Switch Circuit Range/Performance
P0838,Four Wheel Drive (4WD) Switch Circuit Low
P0839,Four Wheel Drive (4WD) Switch Circuit High
P0840,Transmission Fluid Pressure Sensor/Switch A Circuit
P0841,Transmission Fluid Pressure Sensor/Switch A Circuit Range/Performance
P0842,Transmission Fluid Pressure Sensor/Switch A Circuit Low
P0843,Transmission Fluid Pressure Sensor/Switch A Circuit High
P0844,Transmission Fluid Pressure Sensor/Switch A Circuit Intermittent
P0845,Transmission Fluid Pressure Sensor/Switch B Circuit
P0846,Transmission Fluid Pressure Sensor/Switch B Circuit Range/Performance
P0847,Transmission Fluid Pressure Sensor/Switch B Circuit Low
P0848,Transmission Fluid Pressure Sensor/Switch B Circuit High
P0849,Transmission Fluid Pressure Sensor/Switch B Circuit Intermittent
P0850,Park / Neutral Switch Input Circuit
P0851,Park / Neutral Switch Input Circuit Low
P0852,Park / Neutral Switch Input Circuit High
P0853,Drive Switch Input Circuit
P0854,Drive Switch Input Circuit Low
P0855,Drive Switch Input Circuit High
P0856,Traction Control Input Signal
P0857,Traction Control Input Signal Range/Performance
P0858,Traction Control Input Signal Low
P0859,Traction Control Input Signal High
P0860,Gear Shift Module Communication Circuit
P0861,Gear Shift Module Communication Circuit Low
P0862,Gear Shift Module Communication Circuit High
P0863,TCM Communication Circuit
P0864,TCM Communication Circuit Range/Performance
P0865,TCM Communication Circuit Low
P0866,TCM Communication Circuit High
P0867,Transmission Fluid Pressure
P0868,Transmission Fluid Pressure Low
P0869,Transmission Fluid Pressure High
P0870,Transmission Fluid Pressure Sensor/Switch C Circuit
P0871,Transmission Fluid Pressure Sensor/Switch C Circuit Range/Performance
P0872,Transmission Fluid Pressure Sensor/Switch C Circuit Low
P0873,Transmission Fluid Pressure Sensor/Switch C Circuit High
P0874,Transmission Fluid Pressure Sensor/Switch C Circuit Intermittent
P0875,Transmission Fluid Pressure Sensor/Switch D Circuit
P0876,Transmission Fluid Pressure Sensor/Switch D Circuit Range/Performance
P0877,Transmission Fluid Pressure Sensor/Switch D Circuit Low
P0878,Transmission Fluid Pressure Sensor/Switch D Circuit High
P0879,Transmission Fluid Pressure Sensor/Switch D Circuit Intermittent
P0880,TCM Power Input Signal
P0881,TCM Power Input Signal Range/Performance
P0882,TCM Power Input Signal Low
P0883,TCM Power Input Signal High
P0884,TCM Power Input Signal Intermittent
P0885,TCM Power Relay Control Circuit /Open
P0886,TCM Power Relay Control Circuit Low
P0887,TCM Power Relay Control Circuit High
P0888,TCM Power Relay Sense Circuit
P0889,TCM Power Relay Sense Circuit Range/Performance
P0890,TCM Power Relay Sense Circuit Low
P0891,TCM Power Relay Sense Circuit High
P0892,TCM Power Relay Sense Circuit Intermittent
P0893,Multiple Gears Engaged
P0894,Transmission Component Slipping
P0895,Shift Time Too Short
P0896,Shift Time Too Long
P0897,Transmission Fluid Deteriorated
P0898,Transmission Control System MIL Request Circuit Low
P0899,Transmission Control System MIL Request Circuit High
P0900,Clutch Actuator Circuit / Open
P0901,Clutch Actuator Circuit Range/Performance
P0902,Clutch Actuator Circuit Low
P0903,Clutch Actuator Circuit High
P0904,Gate Select Position Circuit [senses left / right position]
P0905,Gate Select Position Circuit Range/Performance
P0906,Gate Select Position Circuit Low
P0907,Gate Select Position Circuit High
P0908,Gate Select Position Circuit Intermittent
P0909,Gate Select Control Error
P0910,Gate Select Actuator Circuit / Open [left / right motion]
P0911,Gate Select Actuator Circuit Range/Performance
P0912,Gate Select Actuator Circuit Low
P0913,Gate Select Actuator Circuit High
P0914,Gear Shift Position Circuit [senses forward / rearward position, odd / even gears]
P0915,Gear Shift Position Circuit Range/Performance
P0916,Gear Shift Position Circuit Low
P0917,Gear Shift Position Circuit High
P0918,Gear Shift Position Circuit Intermittent
P0919,Gear Shift Position Control Error
P0920,Gear Shift Forward Actuator Circuit / Open [forward motion, odd gears, 1,3,5]
P0921,Gear Shift Foward Actuator Circuit Range/Performance
P0922,Gear Shift Foward Actuator Circuit Low
P0923,Gear Shift Foward Actuator Circuit High
P0924,Gear Shift Reverse Actuator Circuit / Open [rearward motion, even gears, 2,4,6]
P0925,Gear Shift Reverse Actuator Circuit Range/Performance
P0926,Gear Shift Reverse Actuator Circuit Low
P0927,Gear Shift Reverse Actuator Circuit High
P0928,Gear Shift Lock Solenoid Circuit / Open
P0929,Gear Shift Lock Solenoid Circuit Range/Performance
P0930,Gear Shift Lock Solenoid Circuit Low
P0931,Gear Shift Lock Solenoid Circuit High
P0932,Hydraulic Pressure Sensor Circuit
P0933,Hydraulic Pressure Sensor Range/Performance
P0934,Hydraulic Pressure Sensor Circuit Low Input
P0935,Hydraulic Pressure Sensor Circuit High Input
P0936,Hydraulic Pressure Sensor Circuit Intermittent
P0937,Hydraulic Oil Temperature Sensor Circuit
P0938,Hydraulic Oil Temperature Sensor Range/Performance
P0939,Hydraulic Oil Temperature Sensor Circuit Low Input
P0940,Hydraulic Oil Temperature Sensor Circuit High Input
P0941,Hydraulic Oil Temperature Sensor Circuit Intermittent
P0942,Hydraulic Pressure Unit
P0943,Hydraulic Pressure Unit Cycling Period Too Short
P0944,Hydraulic Pressure Unit Loss of Pressure
P0945,Hydraulic Pump Relay Circuit / Open
P0946,Hydraulic Pump Relay Circuit Range/Performance
P0947,Hydraulic Pump Relay Circuit Low
P0948,Hydraulic Pump Relay Circuit High
P0949,ASM Adaptive Learning Not Done
P0950,ASM Control Circuit [Up / Down / Auto / etc]
P0951,ASM Control Circuit Range/Performance
P0952,ASM Control Circuit Low
P0953,ASM Control Circuit High
P0954,ASM Control Circuit Intermittent
P0955,ASM Mode Circuit [Perf / Winter / Sport / etc]
P0956,ASM Mode Circuit Range/Performance
P0957,ASM Mode Circuit Low
P0958,ASM Mode Circuit High
P0959,ASM Mode Circuit Intermittent
P0960,Pressure Control Solenoid A Control Circuit / Open
P0961,Pressure Control Solenoid A Control Circuit Range/Performance
P0962,Pressure Control Solenoid A Control Circuit Low
P0963,Pressure Control Solenoid A Control Circuit High
P0964,Pressure Control Solenoid B Control Circuit / Open
P0965,Pressure Control Solenoid B Control Circuit Range/Performance
P0966,Pressure Control Solenoid B Control Circuit Low
P0967,Pressure Control Solenoid B Control Circuit High
P0968,Pressure Control Solenoid C Control Circuit / Open
P0969,Pressure Control Solenoid C Control Circuit Range/Performance
P0970,Pressure Control Solenoid C Control Circuit Low
P0971,Pressure Control Solenoid C Control Circuit High
P0972,Shift Solenoid A Control Circuit Range/Performance
P0973,Shift Solenoid A Control Circuit Low
P0974,Shift Solenoid A Control Circuit High
P0975,Shift Solenoid B Control Circuit Range/Performance
P0976,Shift Solenoid B Control Circuit Low
P0977,Shift Solenoid B Control Circuit High
P0978,Shift Solenoid C Control Circuit Range/Performance
P0979,Shift Solenoid C Control Circuit Low
P0980,Shift Solenoid C Control Circuit High
P0981,Shift Solenoid D Control Circuit Range/Performance
P0982,Shift Solenoid D Control Circuit Low
P0983,Shift Solenoid D Control Circuit High
P0984,Shift Solenoid E Control Circuit Range/Performance
P0985,Shift Solenoid E Control Circuit Low
P0986,Shift Solenoid E Control Circuit High
P0987,Transmission Fluid Pressure Sensor/Switch E Circuit
P0988,Transmission Fluid Pressure Sensor/Switch E Circuit Range/Performance
P0989,Transmission Fluid Pressure Sensor/Switch E Circuit Low
P0990,Transmission Fluid Pressure Sensor/Switch E Circuit High
P0991,Transmission Fluid Pressure Sensor/Switch E Circuit Intermittent
P0992,Transmission Fluid Pressure Sensor/Switch F Circuit
P0993,Transmission Fluid Pressure Sensor/Switch F Circuit Range/Performance
P0994,Transmission Fluid Pressure Sensor/Switch F Circuit Low
P0995,Transmission Fluid Pressure Sensor/Switch F Circuit High
P0996,Transmission Fluid Pressure Sensor/Switch F Circuit Intermittent
P0997,Shift Solenoid F Control Circuit Range/Performance
P0998,Shift Solenoid F Control Circuit Low
P0999,Shift Solenoid F Control Circuit High
P1100,MAF Sensor Intermittent/ Check of all OBDII Systems Not Complete
P1101,MAF Sensor Out Of Self Test Range./KOER Not Able To Complete KOER Aborted
P1102,MAF Sensor In Range But Lower Than Expected
P1103,MAF Sensor In Range But Higher Than Expected
P1104,MAF Ground Malfunction
P1105,Dual Alternator Upper Fault
P1106,Dual Alternator Lower Fault/ Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent High Voltage
P1107,Dual Alternator Lower Circuit Malfunction/ Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent Low Voltage
P1108,Dual Alternator Battery Lamp Circuit Malfunction
P1109,IAT - B Sensor Intermittent
P1110,IAT Sensor (D/C) Open/Short 
P1111,Intake Air Temperature (IAT) Sensor Circuit Intermittent High Voltage 
P1112,Intake Air Temperature (IAT) Sensor Circuit Intermittent Low Voltage 
P1113,IAT Sensor Open/Short 
P1114,Engine Coolant Temperature (ECT) Sensor Circuit Intermittent Low Voltage/IAT - B Circuit Low Input 
P1115,Engine Coolant Temperature (ECT) Sensor Circuit Intermittent High Voltage/IAT - B Circuit High Input 
P1116,Engine Coolant sensor out of range/ECT Sensor Out Of Self Test Range 
P1117,Engine Coolant Sensor intermittent/ECT Sensor Intermittent
P1118,Manifold Absolute Temperature Circuit Low Input
P1119,Manifold Absolute Temperature Circuit High Input
P1120,Throttle position sensor out of range
P1121,Throttle Position (TP) Sensor Circuit Intermittent High Voltage
P1122,Throttle Position (TP) Sensor Circuit Intermittent Low Voltage
P1123,Throttle Position Sensor In Range But Higher Than Expected
P1124,Throttle Position Sensor Out Of Self Test Range
P1125,Throttle position sensor intermittent
P1126,Throttle Position (Narrow Range) Sensor Circuit Malfunction
P1127,Exhaust Not Warm, Downstream O2 Sensor
P1128,Upstream Heated O2 Sensors Swapped
P1129,Downstream Heated O2 Sensors Swapped
P1130,Lack Of HO2S Switch - Adaptive Fuel At Limit
P1131,Lack Of HO2S Switch - Sensor Indicates Lean
P1132,Lack Of HO2S Switch - Sensor Indicates Rich
P1133,HO2S Insufficient Switching Sensor 1
P1134,HO2S Transition Time Ratio Sensor 1
P1135,Pedal Position Sensor A Circuit Intermittent
P1136,Fan Control Circuit Malfunction
P1137,Lack Of HO2S Switch - Sensor Indicates Lean
P1138,Lack Of HO2S12 Switch - Sensor Indicates Rich
P1139,Water In Fuel Indicator Circuit Malfunction
P1140,Water In Fuel Condition
P1141,Fuel Restriction Indicator Circuit Malfunction
P1142,Fuel Restriction Condition
P1143,Air Assist Control Valve Range/Performance
P1144,Air Assist Control Valve Circuit Malfunction
P1150,Lack Of HO2S21 Switch - Adaptive Fuel At Limit
P1151,Lack Of HO2S21 Switch - Sensor Indicates Lean
P1152,Lack Of HO2S21 Switch - Sensor Indicates Rich
P1153,Bank 2 Fuel Control Shifted Lean
P1154,Bank 2 Fuel Control Shifted Rich
P1155,Alternative Fuel Controller
P1156,Fuel Select Switch Malfunction
P1157,Lack Of HO2S22 Switch - Sensor Indicates Lean
P1158,Lack Of HO2S22 Switch - Sensor Indicates Rich
P1159,Fuel Stepper Motor Malfunction
P1166,Air/Fuel Ratio Sensor 1 harness is open or shorted
P1167,Invalid Test,throttle not depressed
P1168,Fuel Rail Sensor In-Range Low Failure
P1169,Fuel Rail Sensor In-Range High Failure
P1170,ESO - Engine Shut Off Solenoid Fault
P1171,Rotor Sensor Fault
P1172,Rotor Control Fault
P1173,Rotor Calibration Fault
P1174,Cam Sensor Fault
P1175,Cam Control Fault
P1176,Cam Calibration Fault
P1177,Synchronization Fault
P1178,( open )
P1180,Fuel Delivery System Malfunction - Low
P1181,Fuel Delivery System Malfunction - High
P1182,Fuel Shut Off Solenoid Malfunction
P1183,Engine Oil Temperature Circuit Malfunction
P1184,Engine Oil Temperature Out Of Self Test Range
P1185,FTS High - Fuel Pump Temperature Sensor High
P1186,FTS Low - Fuel Pump Temperature Sensor Low
P1187,Variant Selection
P1188,Calibration Memory Fault
P1189,Pump Speed Signal Fault
P1190,Calibration Resistor Out Of Range
P1191,Key Line Voltage
P1192,Voltage External
P1193,EGR Drive Overcurrent
P1194,ECU A/D Converter
P1195,SCP HBCC Failed To Initialize
P1196,Key Off Voltage High
P1197,Key Off Voltage Low
P1198,Pump Rotor Control Underfueling
P1199,Fuel Level Input Circuit Low
P1200,Injector Control Circuit
P1201,Injector Circuit Open / Shorted - Cylinder #1
P1202,Injector Circuit Open / Shorted - Cylinder #2
P1203,Injector Circuit Open / Shorted - Cylinder #3
P1204,Injector Circuit Open / Shorted - Cylinder #4
P1205,Injector Circuit Open / Shorted - Cylinder #5
P1206,Injector Circuit Open / Shorted - Cylinder #6
P1209,Injector Control Pressure System Fault
P1210,Injector Control Pressure Above Expected Level
P1211,Injector Control Pressure Sensor Above / Below Desired
P1212,Injector Control Pressure Not Detected During Crank
P1213,Start Injector Circuit Malfunction
P1214,Pedal Position Sensor B Circuit Intermittent
P1215,Pedal Position Sensor C Circuit Low Input
P1216,Pedal Position Sensor C Circuit High Input
P1217,Pedal Position Sensor C Circuit Intermittent
P1218,CID High
P1219,CID Low
P1220,Series Throttle Control System Malfunction
P1221,Traction Control System Malfunction
P1222,Traction Control Output Circuit Malfunction
P1223,Pedal Demand Sensor B Circuit High Input
P1224,Throttle Position Sensor B Out Of Self Test Range
P1225,Needle Lift Sensor Malfunction
P1226,Control Sleeve Sensor Malfunction
P1227,Wastegate Failed Closed (Over Pressure)
P1228,Wastegate Failed Open (Under Pressure)
P1229,Intercooler Pump Driver Fault
P1230,Fuel Pump Low Speed Malfunction
P1231,Fuel Pump Secondary Circuit Low, High Speed
P1232,Fuel Pump Speed Primary Circuit Malfunction
P1233,Fuel Pump Driver Module Off Line
P1234,Fuel Pump Driver Module Off Line
P1235,Fuel Pump Control Out Of Range
P1236,Fuel Pump Control Out Of Range
P1237,Fuel Pump Secondary Circuit Malfunction
P1238,Fuel Pump Secondary Circuit Malfunction
P1239,Speed Fuel Pump Positive Feed Fault
P1240,Sensor Power Supply Malfunction
P1241,Sensor Power Supply Low Input
P1242,Sensor Power Supply High Input
P1243,Second Fuel Pump Faulty or Ground Fault
P1244,Alternator Load Input Failed High
P1245,Alternator Load Input Failed Low
P1246,Alternator Load Input Failed
P1247,Turbo Boost Pressure Low
P1248,Turbo Boost Pressure Not Detected
P1249,Wastegate Control Valve Performance
P1250,PRC Solenoid Circuit Malfunction
P1251,Air Mixture Solenoid Circuit Malfunction
P1252,Pedal Correlation PDS1 and LPDS High
P1253,Pedal Correlation PDS1 and LPDS Low
P1254,Pedal Correlation PDS2 and LPDS High
P1255,Pedal Correlation PDS2 and LPDS Low
P1256,Pedal Correlation PDS1 and HPDS
P1257,Pedal Correlation PDS2 and HPDS
P1258,Pedal Correlation PDS1 and PDS2
P1259,Immobilizer to PCM Signal Error
P1260,THEFT Detected, Vehicle Immobilzed
P1261,Cylinder #1 High To Low Side Short
P1262,Cylinder #2 High To Low Side Short
P1263,Cylinder #3 High To Low Side Short
P1264,Cylinder #4 High To Low Side Short
P1265,Cylinder #5 High To Low Side Short
P1266,Cylinder #6 High To Low Side Short
P1267,Cylinder #7 High To Low Side Short
P1268,Cylinder #8 High To Low Side Short
P1269,Immobilizer Code Not Programmed
P1270,Engine RPM Or Speed Limiter Reached
P1271,Cylinder #1 High To Low Side Open
P1272,Cylinder #2 High To Low Side Open
P1273,Cylinder #3 High To Low Side Open
P1274,Cylinder #4 High To Low Side Open
P1275,Cylinder #5 High To Low Side Open
P1276,Cylinder #6 High To Low Side Open
P1277,Cylinder #7 High To Low Side Open
P1278,Cylinder #8 High To Low Side Open
P1280,Injection Control Pressure Out Of Range Low
P1281,Injection Control Pressure Out Of Range High
P1282,Excessive Injection Control Pressure
P1283,IPR Circuit Failure
P1284,Aborted KOER - ICP Failure
P1285,Cylinder head over temp sensed
P1286,Fuel Pulse In Range But Lower Than Expected
P1287,Fuel Pulse In Range But Higher Than Expected
P1288,Cylinder Head Temp Sensor Out Of Self Test Range
P1289,Cylinder Head Temp Sensor High Input
P1290,Cylinder Head Temp Sensor Low Input
P1291,Injector High Side Short To GND Or VBATT - Bank 1
P1292,Injector High Side Short To GND Or VBATT - Bank 2
P1293,Injector High Side Open - Bank 1
P1294,Injector High Side Open - Bank 2/Target idle not reached
P1295,Multi-faults - Bank 1 - With Low Side Shorts
P1296,Multi-faults - Bank 2 - With Low Side Shorts
P1297,Injector High Sides Shorted Together
P1298,IDM Failure
P1299,Cylinder Head Overtemperature Protection Active
P1300,Boost Calibration Fault
P1301,Boost Calibration High
P1302,Boost Calibration Low
P1303,EGR Calibration Fault
P1304,EGR Calibration High
P1305,EGR Calibration Low
P1306,Kickdown Relay Pull - In Circuit Fault
P1307,Kickdown Relay Hold Circuit Fault
P1308,A/C Clutch Circuit Fault
P1309,Misfire Monitor AICE Chip Fault
P1313,Misfire Rate Catalyst Damage Fault - Bank 1
P1314,Misfire Rate Catalyst Damage Fault - Bank 2
P1315,Persistent Misfire
P1316,Injector Circuit / IDM Codes Detected
P1317,Injector Circuit / IDM Codes Not Updated
P1336,Crank / Cam Sensor Range / Performance
P1340,Camshaft Position Sensor B Circuit Malfunction
P1341,Camshaft Position Sensor B Range / Performance
P1345,SGC (Cam Position) Sensor Circuit Malfunction/ Crankshaft Position - Camshaft Position Correlation
P1346,Fuel Level Sensor B Circuit Malfunction
P1347,Fuel Level Sensor B Range / Performance
P1348,Fuel Level Sensor B Circuit Low
P1349,Fuel Level Sensor B Circuit High
P1350,Fuel Level Sensor B Intermittent/Bypass Line Monitor
P1351,IDM Input Circuit Malfunction/ Ignition Coil Control Circuit High Voltage
P1352,Ignition Coil A Primary Circuit Malfunction
P1353,Ignition Coil B Primary Circuit Malfunction
P1354,Ignition Coil C Primary Circuit Malfunction
P1355,Ignition Coil D Primary Circuit Malfunction
P1360,Ignition Coil A Secondary Circuit Malfunction
P1361,Ignition Control (IC) Circuit Low Voltage
P1362,Ignition Coil C Secondary Circuit Malfunction
P1363,Ignition Coil D Secondary Circuit Malfunction
P1364,Ignition Coil Primary Circuit Failure
P1365,Ignition Coil Secondary Circuit Failure
P1366,Ignition Spare
P1367,Ignition Spare
P1368,Ignition Spare
P1369,Engine Temperature Light Monitor Failure
P1370,Insufficient RMP Increase During Spark Test
P1371,Ignition Coil - Cylinder 1 - Early Activation Fault
P1372,Ignition Coil - Cylinder 2 - Early Activation Fault
P1373,Ignition Coil - Cylinder 3 - Early Activation Fault
P1374,Crankshaft Position (CKP)/Ignition Coil - Cylinder 4 - Early Activation Fault
P1375,Ignition Coil - Cylinder 5 - Early Activation Fault
P1376,Ignition Coil - Cylinder 6 - Early Activation Fault
P1380,Misfire Detected - Rough Road Data Not Available
P1381,Variable Cam Timing Overadvanced (Bank #1)/ Misfire Detected - No Communication with BCM
P1382,Variable Cam Timing Solenoid #1 Circuit Malfunction
P1383,Variable Cam Timing Overretarded (Bank #1)
P1384,VVT Solenoid A Malfunction
P1385,Variable Cam Timing Solenoid B Malfunction
P1386,Variable Cam Timing Overadvanced (Bank #2)
P1387,Variable Cam Timing Solenoid #2 Circuit Malfunction
P1388,Variable Cam Timing Overretarded (Bank #2)
P1389,Glow Plug Circuit High Side Low Input
P1390,Octane Adjust Pin Out Of Self Test Range
P1391,Glow Plug Circuit Low Input (Bank #1)
P1392,Glow Plug Circuit High Input (Bank #1)
P1393,Glow Plug Circuit Low Input (Bank #2)
P1394,Glow Plug Circuit High Input (Bank #2)
P1395,Glow Plug Monitor Fault (Bank #1)
P1396,Glow Plug Monitor Fault (Bank #2)
P1397,System Voltage Out Of Self Test Range
P1398,VVT Solenoid B Circuit High Input
P1399,Glow Plug Circuit High Side, High Input
P1400,DPFE Circuit Low Input
P1401,DPFE Circuit High Input
P1402,EGR Metering Orifice Restricted
P1403,DPFE Sensor Hoses Reversed
P1404,IAT - B Circuit Malfunction/ Exhaust Gas Recirculation Closed Position Performance
P1405,DPFE Sensor Upstream Hose Off Or Plugged
P1406,Exhaust Gas Recirculation (EGR) Position Sensor Performance
P1407,EGR No Flow Detected
P1408,EGR Flow Out Of Self Test Range
P1409,EVR Control Circuit Malfunction
P1411,SAI System Incorrect Downstream Flow Detected
P1413,SAI System Monitor Circuit Low Input
P1414,SAI System Monitor Circuit High Input
P1415,Air Pump Circuit Malfunction/ (AIR) System Bank 1
P1416,Port Air Circuit Malfunction/ (AIR) System Bank 2
P1417,Port Air Relief Circuit Malfunction
P1418,Split Air #1 Circuit Malfunction
P1419,Split Air #2 Circuit Malfunction
P1420,Catalyst Temperature Sensor Failure
P1421,Catalyst Damage
P1422,EGI Temperature Sensor Failure
P1423,EGI Functionality Test Failed
P1424,EGI Glow Plug Primary Failure
P1425,EGI Glow Plug Secondary Failure
P1426,EGI Mini - MAF Failed Out Of Range
P1427,EGI Mini - MAF Failed Short Circuit
P1428,EGI Mini - MAF Failed Open Circuit
P1429,Electric Air Pump Primary Failure
P1430,Electric Air Pump Secondary Failure
P1433,A/C Refrigerant Temperature Circuit Low
P1434,A/C Refrigerant Temperature Circuit High
P1435,A/C Refrigerant Temperature Circuit Range/Performance
P1436,A/C Evaporator Air Temperature Circuit Low
P1437,A/C Evaporator Air Temperature Circuit High
P1438,A/C Evaporator Air Temperature Circuit Range/Performance
P1439,Floor Temperature Switch Circuit Malfunction
P1440,Purge Valve Stuck Open
P1441,Evaporative Emission (EVAP) System Flow During Non-Purge Chevrolet Only
P1442,Evaporative Emission Control System Leak Detected
P1443,Evaporative Emission Control System Control Valve
P1444,Purge Flow Sensor Circuit Low Input
P1445,Purge Flow Sensor Circuit High Input
P1446,Evaporative Vac Solenoid Circuit Malfunction
P1447,ELC System Closure Valve Flow Fault
P1448,ELC System 2 Fault
P1449,Evaporative Check Solenoid Circuit Malfunction
P1450,Unable To Bleed Up Fuel Tank Vacuum
P1451,Evap Emission Control Sys Vent Control Valve Circuit
P1452,Unable To Bleed - Up Vacuum in Tank
P1453,Fuel Tank Pressure Relief Valve Malfunction
P1454,Evaporative System Vacuum Test Malfunction
P1455,Evap Emission Control Sys Leak Detected (Gross Leak/No Flow)
P1456,Fuel Tank Temperature Sensor Circuit Malfunction
P1457,Unable To Pull Vacuum In Tank
P1460,Wide open throttle A/C cutoff relay circuit
P1461,A/C pressure sensor circuit voltage low
P1462,A/C pressure sensor circuit voltage high
P1463,A/C Pressure Sensor Insufficient Pressure Change
P1464,A/C Demand Out of Self Test Range
P1465,A/C Relay Circuit Malfunction
P1466,A/C Refrigerant Temperature Sensor/Circuit Malfunction
P1467,A/C Compressor Temperature Sensor Malfunction
P1468,SSPOD Open Circuit or Closed Circuit Fault
P1469,Low A/C Cycling Period
P1470,A/C Cycling Period Too Short
P1471,Electrodrive Fan 1 Operational Failure (Driver Side)
P1472,Electrodrive Fan 2 Operational Failure (Passenger Side)
P1473,Fan Secondary High With Fan(s) Off
P1474,Low Fan Control Primary Circuit Malfunction
P1475,Fan Relay (Low) Circuit Malfunction
P1476,Fan Relay (High) Circuit Malfunction
P1477,Additional Fan Relay Circuit Malfunction
P1478,Cooling Fan Driver Fault
P1479,High Fan Control Primary Circuit Malfunction
P1480,Fan Secondary Low with Low Fan On
P1481,Fan Secondary Low With High Fan On
P1482,SCP
P1483,Power To Fan Circuit Overcurrent
P1484,Open Power To Ground VCRM
P1485,EGRV Circuit Malfunction
P1486,EGRA Circuit Malfunction
P1487,EGRCHK Solenoid Circuit Malfunction
P1490,Secondary Air Relief Solenoid Circuit Malfunction
P1491,Secondary Switch Solenoid Circuit Malfunction
P1492,APLSOL Solenoid Circuit Malfunction
P1493,RCNT Solenoid Circuit Malfunction
P1494,SPCUT Solenoid Circuit Malfunction
P1495,TCSPL Solenoid Circuit Malfunction
P1500,Vehicle Speed Sensor Intermittent
P1501,Vehicle Speed Sensor Out Of Self Test Range
P1502,Vehicle Speed Sensor Intermittent Malfunction
P1503,Auxillary Speed Sensor Fault
P1504,Idle Air Control Circuit Malfunction
P1505,Idle Air Control System At Adaptive Clip
P1506,Idle Air Control Overspeed Error
P1507,Idle Air Control Underspeed Error
P1508,Idle Control System Circuit Open
P1509,Idle Control System Circuit Shorted
P1510,Idle Signal Circuit Malfunction
P1511,Idle Switch (Electric Control Throttle) Circuit Malfunction
P1512,Intake Manifold Runner Control (Bank 1) Stuck Closed
P1513,Intake Manifold Runner Control (Bank 2) Stuck Closed
P1514,High Load Neutral/Drive Fault
P1515,Electric Current Circuit Malfunction
P1516,IMRC Input Error (Bank 1)
P1517,IMRC Input Error (Bank 2)
P1518,Intake Manifold Runner Control (Stuck Open)
P1519,Intake Manifold Runner Control (Stuck Closed)
P1520,Intake Manifold Runner Control Circuit Malfunction
P1521,Variable Intake Solenoid #1 Circuit Malfunction
P1522,Variable Intake Solenoid #2 Circuit Malfunction
P1523,IVC Solenoid Circuit Malfunction
P1524,Variable Intake Solenoid System
P1525,Air Bypass Valve System
P1526,Air Bypass System
P1527,Accelerate Warmup Solenoid Circuit Malfunction
P1528,Subsidiary Throttle Valve Solenoid Circuit Malfunction
P1529,SCAIR Solenoid Circuit Malfunction
P1530,A/C Clutch Circuit Malfunction
P1531,Invalid Test - Accelerator Pedal Movement
P1532,IMCC Circuit Malfunction, Bank B
P1533,AAI Circuit Malfunction
P1534,Inertia Switch Activated
P1535,Blower Fan Speed Circuit Range/Performance
P1536,Parking Brake Switch Circuit Failure
P1537,Intake Manifold Runner Control (Bank 1) Stuck Open
P1538,Intake Manifold Runner Control (Bank 2) Stuck Open
P1539,Power To A/C Clutch Circuit Overcurrent
P1540,Air Bypass Valve Circuit Malfunction
P1549,IMCC Circuit Malfunction, Bank B
P1550,PSPS Out Of Self Test Range
P1565,Speed Control Command Switch Out of Range High
P1566,Speed Control Command Switch Out of Range Low
P1567,Speed Control Output Circuit Continuity
P1568,Speed Control Unable to Hold Speed
P1571,Brake Switch Malfunction
P1572,Brake Pedal Switch Circuit Malfunction
P1573,Throttle Position Not Available
P1574,Throttle Position Sensor Disagreement btwn Sensors
P1575,Pedal Position Out of Self Test Range
P1576,Pedal Position Not Available
P1577,Pedal Position Sensor Disagreement btwn Sensors
P1578,ETC Power Less Than Demand
P1579,ETC In Power Limiting Mode
P1580,Electronic Throttle Monitor PCM Override
P1581,Electronic Throttle Monitor Malfunction
P1582,Electronic Throttle Monitor Data Available
P1583,Electronic Throttle Monitor Cruise Disable
P1584,TCU Detected IPE Circuit Malfunction
P1585,Throttle Control Unit Malfunction
P1586,Throttle Control Unit Throttle Position Malfunction
P1587,Throttle Control Unit Modulated Command Malfunction
P1588,Throttle Control Unit Detected Loss of Return Spring
P1589,TCU Unable To Control Desired Throttle Angle
P1600,Loss of KAM Power; Open Circuit
P1601,ECM/TCM Serial Communication Error
P1602,Immobilizer/ECM Communication Error
P1603,EEPROM Malfunction
P1604,Code Word Unregestered
P1605,Keep Alive Memory Test Failure
P1606,ECM Control Relay O/P Circuit Malfunction
P1607,MIL O/P Circuit Malfunction
P1608,Internal ECM Malfunction
P1609,Diagnostic Lamp Driver Fault
P1610,SBDS Interactive Codes
P1611,SBDS Interactive Codes
P1612,SBDS Interactive Codes
P1613,SBDS Interactive Codes
P1614,SBDS Interactive Codes
P1615,SBDS Interactive Codes
P1616,SBDS Interactive Codes
P1617,SBDS Interactive Codes
P1618,SBDS Interactive Codes
P1619,SBDS Interactive Codes
P1620,SBDS Interactive Codes
P1621,Control Module Long Term Memory Performance/ Immobilizer Code Words Do Not Match
P1622,Immobilizer ID Does Not Match
P1623,Immobilizer Code Word/ID Number Write Failure
P1624,Anti Theft System
P1625,B+ Supply To VCRM Fan Circuit Malfunction
P1626,Theft Deterrent Fuel Enable Signal Not Received/ B+ Supply To VCRM A/C Circuit Malfunction
P1627,Module Supply Voltage Out Of Range
P1628,Module Ignition Supply Input Malfunction
P1629,Internal Voltage Regulator Malfunction
P1630,Internal Vref Malfunction
P1631,Theft Deterrent Start Enable Signal Not Correct/ Main Relay Malfunction (Power Hold)
P1632,Smart Alternator Faults Sensor/Circuit Malfunction
P1633,KAM Voltage Too Low
P1634,Data Output Link Circuit Failure
P1635,Tire / Axle Ratio Out of Acceptable Range
P1636,Inductive Signature Chip Communication Error
P1637,Can Link ECM/ABSCM Circuit / Network Malfunction
P1638,Can Link ECM/INSTM Circuit / Network Malfunction
P1639,Vehicle ID Block Corrupted or Not Programmed
P1640,Powertrain DTCs Available in Another Module
P1641,Fuel Pump Primary Circuit Failure
P1642,Fuel Pump Monitor Circuit High Input
P1643,Fuel Pump Monitor Circuit Low Input
P1644,Fuel Pump Speed Control Circuit Malfunction
P1645,Fuel Pump Resistor Switch Circuit Malfunction
P1650,PSP Switch Out of Self Test Range
P1651,PSP Switch Input Malfunction
P1652,IAC Monitor Disabled by PSP Switch Failed On
P1653,Power Steering Output Circuit Malfunction
P1654,Recirculation Override Circuit Malfunction
P1655,Starter Disable Circuit Malfunction
P1660,Output Circuit Check Signal High
P1661,Output Circuit Check Signal Low
P1662,IDM_EN Circuit Failure
P1663,Fuel Demand Command Signal Circuit Malfunction
P1667,CI Circuit Malfunction
P1668,PCM - IDM Communications Error
P1670,Electronic Feedback Signal Not Detected
P1680,Metering Oil Pump Malfunction
P1681,Metering Oil Pump Malfunction
P1682,Metering Oil Pump Malfunction
P1683,Metering Oil Pump Temperature Sensor Circuit Malfunction
P1684,Metering Oil Pump Position Sensor Circuit Malfunction
P1685,Metering Oil Pump Stepping Motor Circuit Malfunction
P1686,Metering Oil Pump Stepping Motor Circuit Malfunction
P1687,Metering Oil Pump Stepping Motor Circuit Malfunction
P1688,Metering Oil Pump Stepping Motor Circuit Malfunction
P1689,Oil Pressure Control Solenoid Circuit Malfunction
P1690,Wastegate Solenoid Circuit Malfunction
P1691,Turbo Pressure Control Solenoid Circuit Malfunction
P1692,Turbo Control Solenoid Circuit Malfunction
P1693,Turbo Charge Control Circuit Malfunction
P1694,Turbo Charge Relief Circuit Malfunction
P1700,Transmission Indeterminate Failure (Failed to Neutral)
P1701,Reverse Engagement Error
P1702,TRS Circuit Intermittent Malfunction
P1703,Brake Switch Out Of Self Test Range
P1704,Digital TRS Failed to Transition States in KOEO / KOER
P1705,Not in P or N During KOEO / KOER
P1706,High Vehicle Speed Observed in Park
P1707,Transfer Case Neutral Indicator Hard Fault Present
P1708,Clutch Switch Circuit Malfunction
P1709,PNP Switch Out Of Self Test Range
P1711,TFT Sensor Out Of Self Test Range
P1712,Trans Torque Reduction Request Signal Malfunction
P1713,TFT Sensor In Range Failure Low Value
P1714,SSA Inductive Signature Malfunction
P1715,SSB Inductive Signature Malfunction
P1716,SSC Inductive Signature Malfunction
P1717,SSD Inductive Signature Malfunction
P1718,TFT Sensor In Range Failure High
P1720,Vehicle Speed (Meter) Circuit Malfunction
P1721,Gear 1 Incorrect Ratio
P1722,Gear 2 Incorrect Ratio
P1723,Gear 3 incorrect Ratio
P1724,Gear 4 Incorrect Ratio
P1725,Insufficient Engine Speed Increase During Self Test
P1726,Insufficient Engine Speed Decrease During Self Test
P1727,Coast Clutch Solenoid Inductive Signature Malfunction
P1728,Transmission Slip Error
P1729,4x4 Low Switch Error
P1730,Gear Control Malfunction 2,3,5
P1731,1-2 Shift Malfunction
P1732,2-3 Shift Malfunction
P1733,3-4 Shift Malfunction
P1734,Gear Control Malfunction
P1735,First Gear Switch Circuit Malfunction
P1736,Second Gear Switch Circuit Malfunction
P1737,Lockup Solenoid System
P1738,Shift Time Error
P1739,Slip Solenoid System
P1740,Torque Converter Clutch Inductive Signature Malfunction
P1741,Torque Converter Clutch Control Error
P1742,Torque Converter Clutch Solenoid Failed On
P1743,Torque Converter Clutch Solenoid Failied On
P1744,Torque Converter Clutch System Performance
P1745,Line Pressure Solenoid System
P1746,Pressure Control Solenoid 'A' Open Circuit
P1747,Pressure Control Solenoid 'A' Short Circuit
P1748,EPC Malfunction
P1749,Pressure Control Solenoid Failed Low
P1751,Shift Solenoid A Performance
P1753,Torque Converter Clutch Solenoid Valve Circuit
P1754,Coast Clutch Solenoid Circuit Malfunction
P1755,Intermediate Speed Sensor (ISS) Malfunction
P1756,Shift Solenoid B Performance
P1760,Pressure Control Solenoid 'A' Short Circuit
P1761,Shift Solenoid C Performance
P1762,Overdrive Band Failed Off
P1765,Timing Solenoid Circuit Malfunction
P1767,Torque Converter Clutch Circuit Malfunction
P1768,Performance / Normal / Winter Mode Input Malfunction
P1769,AG4 Transmission Torque Modulation Fault
P1770,Clutch Solenoid Circuit Malfunction
P1775,Transmission System MIL Fault
P1776,Ignition Retard Request Duration Fault
P1777,Ignition Retard Request Circuit Fault
P1778,Transmission Reverse I/P Circuit Malfunction
P1779,TCIL Circuit Malfunction
P1780,Trans Control Switch (O/D Cancel) Out of Self Test Range
P1781,4X4 Switch Out of Self Test Range
P1782,P/ES Circuit Out Of Self Test Range
P1783,Transmission Overtemperature Condition
P1784,Transmission Mechanical Failure - First And Reverse
P1785,Transmission Mechanical Failure - First And Second
P1786,3-2 Downshift Error
P1787,2-1 Downshift Error
P1788,Pressure Control Solenoid 'B' Open Circuit
P1789,Pressure Control Solenoid 'B' Short Circuit
P1790,TP (Mechanical) Circuit Malfunction
P1791,TP (Electric) Circuit Malfunction
P1792,Barometer Pressure Circuit Malfunction
P1793,Intake Air Volume Circuit Malfunction
P1794,Battery Voltage Circuit Malfunction
P1795,Idle Switch Circuit Malfunction
P1796,Kick Down Switch Circuit Malfunction
P1797,Neutral Switch Circuit Malfunction
P1798,Coolant Temperature Circuit Malfunction
P1799,Hold Switch Circuit Malfunction
P1800,Transmission Clutch Interlock Safety Switch Circuit Failure
P1801,Transmission Clutch Interlock Safety Switch Open Circuit
P1802,Transmission Clutch Interlock Safety Switch Short Circuit To Battery
P1803,Transmission Clutch Interlock Safety Switch Short Circuit To Ground
P1804,Transmission 4-Wheel Drive High Indicator Circuit Failure
P1805,Transmission 4-Wheel Drive High Indicator Open Circuit
P1806,Transmission 4-Wheel Drive High Indicator Short Circuit To Battery
P1807,Transmission 4-Wheel Drive High Indicator Short Circuit To Ground
P1808,Transmission 4-Wheel Drive Low Indicator Circuit Failure
P1809,Transmission 4-Wheel Drive Low Indicator Open Circuit
P1810,TFP Valve Position Switch Circuit/ Transmission 4-Wheel Drive Low Indicator Short Circuit To Battery
P1811,Transmission 4-Wheel Drive Low Indicator Short Circuit To Ground
P1812,Transmission 4-Wheel Drive Mode Select Circuit Failure
P1813,Transmission 4-Wheel Drive Mode Select Open Circuit
P1814,Transmission 4-Wheel Drive Mode Select Short Circuit To Battery
P1815,Transmission 4-Wheel Drive Mode Select Short Circuit To Ground
P1816,Transmission Neutral Safety Switch Circuit Failure
P1817,Transmission Neutral Safety Switch Open Circuit
P1818,Transmission Neutral Safety Switch Short Circuit To Battery
P1819,Transmission Neutral Safety Switch Short Circuit To Ground
P1820,Transmission Transfer Case Clockwise Shift Relay Coil Circuit Failure
P1821,Transmission Transfer Case Clockwise Shift Relay Coil Open Circuit
P1822,Transmission Transfer Case Clockwise Shift Relay Coil Short Circuit To Battery
P1823,Transmission Transfer Case Clockwise Shift Relay Coil Short Circuit To Ground
P1824,Transmission 4-Wheel Drive Clutch Relay Circuit Failure
P1825,Transmission 4-Wheel Drive Clutch Relay Open Circuit
P1826,Transmission 4-Wheel Drive Low Clutch Relay Circuit To Battery
P1827,Transmission 4-Wheel Drive Low Clutch Relay Circuit To Ground
P1828,Transmission Transfer Case Counter Clockwise Shift Relay Coil Circuit Failure
P1829,Transmission Transfer Case Counter Clockwise Shift Relay Coil Open Circuit
P1830,Transmission Transfer Case Counter Clockwise Shift Relay Coil Short Circuit To Battery
P1831,Transmission Transfer Case Counter Clockwise Shift Relay Coil Short Circuit To Ground
P1832,Transmission Transfer Case Differential Lock-Up Solenoid Circuit Failure
P1833,Transmission Transfer Case Differential Lock-Up Solenoid Open Circuit
P1834,Transmission Transfer Case Differential Lock-Up Solenoid Short Circuit To Battery
P1835,Transmission Transfer Case Differential Lock-Up Solenoid Short Circuit To Ground
P1836,Transmission Transfer Case Front Shaft Speed Sensor Circuit Failure
P1837,Transmission Transfer Case Rear Shaft Speed Sensor Circuit Failure
P1838,Transmission Transfer Case Shift Motor Circuit Failure
P1839,Transmission Transfer Case Shift Motor Open Circuit
P1840,Transmission Transfer Case Shift Motor Short Circuit To Battery
P1841,Transmission Transfer Case Shift Motor Short Circuit To Ground
P1842,Transmission Transfer Case Differential Lock-Up Feedback Switch Circuit Failure
P1843,Transmission Transfer Case Differential Lock-Up Feedback Switch Open Circuit
P1844,Transmission Transfer Case Differential Lock-Up Feedback Switch Short Circuit To Battery
P1845,Transmission Transfer Case Differential Lock-Up Feedback Switch Short Circuit To Ground
P1846,Transmission Transfer Case Contact Plate 'A' Circuit Failure
P1847,Transmission Transfer Case Contact Plate 'A' Open Circuit
P1848,Transmission Transfer Case Contact Plate 'A' Short Circuit To Battery
P1849,Transmission Transfer Case Contact Plate 'A' Short Circuit To Ground
P1850,Transmission Transfer Case Contact Plate 'B' Circuit Failure
P1851,Transmission Transfer Case Contact Plate 'B' Open Circuit
P1852,Transmission Transfer Case Contact Plate 'B' Short Circuit To Battery
P1853,Transmission Transfer Case Contact Plate 'B' Short Circuit To Ground
P1854,Transmission Transfer Case Contact Plate 'C' Circuit Failure
P1855,Transmission Transfer Case Contact Plate 'C' Open Circuit
P1856,Transmission Transfer Case Contact Plate 'C' Short Circuit To Battery
P1857,Transmission Transfer Case Contact Plate 'C' Short Circuit To Ground
P1858,Transmission Transfer Case Contact Plate 'D' Circuit Failure
P1859,Transmission Transfer Case Contact Plate 'D' Open Circuit
P1860,TCC PWM Solenoid Circuit Electrical/ Transmission Transfer Case Contact Plate 'D' Short Circuit To Battery
P1861,Transmission Transfer Case Contact Plate 'D' Short Circuit To Ground
P1862,Transmission Transfer Case Contact Plate Power Circuit Failure
P1863,Transmission Transfer Case Contact Plate Power Open Circuit
P1864,Transmission Transfer Case Contact Plate Power Short To Battery
P1865,Transmission Transfer Case Contact Plate Power Short To Ground
P1866,Transmission Transfer Case System Concern - Servicing Required
P1867,Transmission Transfer Case Contact Plate General Circuit Failure
P1868,Transmission Automatic 4-Wheel Drive Indicator (Lamp) Circuit Failure
P1869,Transmission Automatic 4-Wheel Drive Indicator (Lamp) Circuit Short To Battery
P1870,Transmission Component Slipping/ Transmission Mechanical Transfer Case 4x4 Switch Circuit Failure
P1871,Transmission Mechanical Transfer Case 4x4 Switch Circuit Short To Battery
P1872,Transmission Mechanical 4-Wheel Drive Axle Lock Lamp Circuit Failure
P1873,Transmission Mechanical 4-Wheel Drive Axle Lock Lamp Circuit Short To Battery
P1874,Transmission Automatic Hall Effect Sensor Power Circuit Failure
P1875,Transmission Automatic Hall Effect Sensor Power Circuit Short To Battery / 4WD Low Switch Circuit Electrical
P1876,Transmission Transfer Case 2-Wheel Drive Solenoid Circuit Failure
P1877,Transmission Transfer Case 2-Wheel Drive Solenoid Circuit Short To Battery
P1878,Transmission Transfer Case Disengaged Solenoid Circuit Failure
P1879,Transmission Transfer Case Disengaged Solenoid Open Circuit
P1880,Transmission Transfer Case Disengaged Solenoid Short to Battery
P1881,Engine Coolant Level Switch Circuit Failure, GEM
P1882,Engine Coolant Level Switch Circuit Short to Ground
P1883,Engine Coolant Level Switch Circuit Failure, GEM
P1884,Engine Coolant Level Lamp Circuit Short to Ground
P1885,Transmission Transfer Case Disengaged Solenoid Short to Ground
P1886,4X4 Initialization Failure
P1890,Transmission 4WD Mode Select Return Input Circuit Failure
P1891,Transmission Transfer Case Contact Plate Ground Return Open Circuit
P1900,OSS Circuit Intermittent Malfunction
P1901,TSS Circuit Intermittent Malfunction
P1902,Pressure Control Solenoid 'B' Intermittent Short
P1903,Pressure Control Solenoid 'C' Short Circuit
P1904,Pressure Control Solenoid 'C' Open Circuit
P1905,Pressure Control Solenoid 'C' Intermittent Short
P1906,Kickdown Pull Relay Open or Short Circuit to Ground
P1907,Kickdown Hold Relay Open or Short Circuit to Ground
P1908,Transmission Pressure Circuit Solenoid Open or Short to Ground
P1909,Trans Temp Sensor Circuit Open or Shorted to Pwr or Gnd
P1910,VFS A Pressure Output Failed Low
P1911,VFS B Pressure Output Failed Low
P1912,VFS C Pressure Output Failed Low
P1913,Pressure Switch A Circuit Malfunction
P1914,Manually Shifted Automatic (MSA) Sw Circuit Malf
P1915,Reverse Switch Circuit Malfunction
P1916,High Clutch Drum Speed Sensor Malfunction
P1917,High Clutch Drum Speed Sensor Intermittent
P1918,Transmission Range Display Circuit Malfunction