(kicad_symbol_lib (version 20201005) (generator kicad_symbol_editor)
  (symbol "mcu:Module-mcu-0.5" (in_bom yes) (on_board yes)
    (property "Reference" "M" (id 0) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Module-mcu-0.5" (id 1) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "hellen-one-mcu-0.5:mcu" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Hellen One MCU Module" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Module-mcu-0.5_1_0"
      (rectangle (start 15.24 0) (end 0 -114.3)
        (stroke (width 0)) (fill (type background))
      )
      (pin passive line (at 20.32 -2.54 180) (length 5.08)
        (name "SPI1_SCK" (effects (font (size 1.27 1.27))))
        (number "E1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -5.08 180) (length 5.08)
        (name "SPI1_MISO" (effects (font (size 1.27 1.27))))
        (number "E2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -7.62 180) (length 5.08)
        (name "SPI1_MOSI" (effects (font (size 1.27 1.27))))
        (number "E3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -10.16 180) (length 5.08)
        (name "SPI1_CS1" (effects (font (size 1.27 1.27))))
        (number "E4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -12.7 180) (length 5.08)
        (name "SPI1_CS2" (effects (font (size 1.27 1.27))))
        (number "E5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -58.42 180) (length 5.08)
        (name "CAN_VIO" (effects (font (size 1.27 1.27))))
        (number "N1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -43.18 180) (length 5.08)
        (name "SPI3_MISO" (effects (font (size 1.27 1.27))))
        (number "N10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -45.72 180) (length 5.08)
        (name "SPI3_MOSI" (effects (font (size 1.27 1.27))))
        (number "N11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -68.58 180) (length 5.08)
        (name "I2C_SDA" (effects (font (size 1.27 1.27))))
        (number "N18" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -71.12 180) (length 5.08)
        (name "I2C_SCL" (effects (font (size 1.27 1.27))))
        (number "N19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -60.96 180) (length 5.08)
        (name "CAN_RX" (effects (font (size 1.27 1.27))))
        (number "N2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -22.86 180) (length 5.08)
        (name "SPI2_SCK" (effects (font (size 1.27 1.27))))
        (number "N20" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -25.4 180) (length 5.08)
        (name "SPI2_MISO" (effects (font (size 1.27 1.27))))
        (number "N21" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -27.94 180) (length 5.08)
        (name "SPI2_MOSI" (effects (font (size 1.27 1.27))))
        (number "N22" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -30.48 180) (length 5.08)
        (name "SPI2_CS" (effects (font (size 1.27 1.27))))
        (number "N23" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -106.68 180) (length 5.08)
        (name "SWCLK" (effects (font (size 1.27 1.27))))
        (number "N25" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -109.22 180) (length 5.08)
        (name "SWDIO" (effects (font (size 1.27 1.27))))
        (number "N26" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -111.76 180) (length 5.08)
        (name "SWO" (effects (font (size 1.27 1.27))))
        (number "N27" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -101.6 180) (length 5.08)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "N29" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -63.5 180) (length 5.08)
        (name "CAN_TX" (effects (font (size 1.27 1.27))))
        (number "N3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -93.98 180) (length 5.08)
        (name "USB1P" (effects (font (size 1.27 1.27))))
        (number "N30" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -96.52 180) (length 5.08)
        (name "USB1M" (effects (font (size 1.27 1.27))))
        (number "N31" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -99.06 180) (length 5.08)
        (name "USB1ID" (effects (font (size 1.27 1.27))))
        (number "N32" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -81.28 180) (length 5.08)
        (name "UART1_TX" (effects (font (size 1.27 1.27))))
        (number "N4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -78.74 180) (length 5.08)
        (name "UART1_RX" (effects (font (size 1.27 1.27))))
        (number "N5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -88.9 180) (length 5.08)
        (name "UART2_TX" (effects (font (size 1.27 1.27))))
        (number "N6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -86.36 180) (length 5.08)
        (name "UART2_RX" (effects (font (size 1.27 1.27))))
        (number "N7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -48.26 180) (length 5.08)
        (name "SPI3_CS" (effects (font (size 1.27 1.27))))
        (number "N8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -40.64 180) (length 5.08)
        (name "SPI3_SCK" (effects (font (size 1.27 1.27))))
        (number "N9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "Module-mcu-0.5_2_0"
      (rectangle (start 15.24 0) (end 0 -109.22)
        (stroke (width 0)) (fill (type background))
      )
      (pin passive line (at 20.32 -99.06 180) (length 5.08)
        (name "OUT_IO10" (effects (font (size 1.27 1.27))))
        (number "E10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -96.52 180) (length 5.08)
        (name "OUT_IO9" (effects (font (size 1.27 1.27))))
        (number "E11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -78.74 180) (length 5.08)
        (name "OUT_IO2" (effects (font (size 1.27 1.27))))
        (number "E12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -104.14 180) (length 5.08)
        (name "OUT_IO12" (effects (font (size 1.27 1.27))))
        (number "E13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -55.88 180) (length 5.08)
        (name "OUT_PWM2" (effects (font (size 1.27 1.27))))
        (number "E14" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -58.42 180) (length 5.08)
        (name "OUT_PWM3" (effects (font (size 1.27 1.27))))
        (number "E15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -60.96 180) (length 5.08)
        (name "OUT_PWM4" (effects (font (size 1.27 1.27))))
        (number "E16" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -63.5 180) (length 5.08)
        (name "OUT_PWM5" (effects (font (size 1.27 1.27))))
        (number "E17" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -66.04 180) (length 5.08)
        (name "OUT_PWM6" (effects (font (size 1.27 1.27))))
        (number "E18" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -68.58 180) (length 5.08)
        (name "OUT_PWM7" (effects (font (size 1.27 1.27))))
        (number "E19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -101.6 180) (length 5.08)
        (name "OUT_IO11" (effects (font (size 1.27 1.27))))
        (number "E20" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -91.44 180) (length 5.08)
        (name "OUT_IO7" (effects (font (size 1.27 1.27))))
        (number "E21" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -93.98 180) (length 5.08)
        (name "OUT_IO8" (effects (font (size 1.27 1.27))))
        (number "E22" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -83.82 180) (length 5.08)
        (name "OUT_IO4" (effects (font (size 1.27 1.27))))
        (number "E23" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -106.68 180) (length 5.08)
        (name "OUT_IO13" (effects (font (size 1.27 1.27))))
        (number "E24" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -30.48 180) (length 5.08)
        (name "OUT_INJ1" (effects (font (size 1.27 1.27))))
        (number "E25" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -33.02 180) (length 5.08)
        (name "OUT_INJ2" (effects (font (size 1.27 1.27))))
        (number "E26" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -53.34 180) (length 5.08)
        (name "OUT_PWM1" (effects (font (size 1.27 1.27))))
        (number "E27" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -71.12 180) (length 5.08)
        (name "OUT_PWM8" (effects (font (size 1.27 1.27))))
        (number "E28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -35.56 180) (length 5.08)
        (name "OUT_INJ3" (effects (font (size 1.27 1.27))))
        (number "E29" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -38.1 180) (length 5.08)
        (name "OUT_INJ4" (effects (font (size 1.27 1.27))))
        (number "E30" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -40.64 180) (length 5.08)
        (name "OUT_INJ5" (effects (font (size 1.27 1.27))))
        (number "E31" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -43.18 180) (length 5.08)
        (name "OUT_INJ6" (effects (font (size 1.27 1.27))))
        (number "E32" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -45.72 180) (length 5.08)
        (name "OUT_INJ7" (effects (font (size 1.27 1.27))))
        (number "E33" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -48.26 180) (length 5.08)
        (name "OUT_INJ8" (effects (font (size 1.27 1.27))))
        (number "E34" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -81.28 180) (length 5.08)
        (name "OUT_IO3" (effects (font (size 1.27 1.27))))
        (number "E6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -86.36 180) (length 5.08)
        (name "OUT_IO5" (effects (font (size 1.27 1.27))))
        (number "E7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -76.2 180) (length 5.08)
        (name "OUT_IO1" (effects (font (size 1.27 1.27))))
        (number "E8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -88.9 180) (length 5.08)
        (name "OUT_IO6" (effects (font (size 1.27 1.27))))
        (number "E9" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -2.54 180) (length 5.08)
        (name "OUT_IGN1" (effects (font (size 1.27 1.27))))
        (number "W1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -5.08 180) (length 5.08)
        (name "OUT_IGN2" (effects (font (size 1.27 1.27))))
        (number "W2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -7.62 180) (length 5.08)
        (name "OUT_IGN3" (effects (font (size 1.27 1.27))))
        (number "W3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -10.16 180) (length 5.08)
        (name "OUT_IGN4" (effects (font (size 1.27 1.27))))
        (number "W4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -12.7 180) (length 5.08)
        (name "OUT_IGN5" (effects (font (size 1.27 1.27))))
        (number "W5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -15.24 180) (length 5.08)
        (name "OUT_IGN6" (effects (font (size 1.27 1.27))))
        (number "W6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -17.78 180) (length 5.08)
        (name "OUT_IGN7" (effects (font (size 1.27 1.27))))
        (number "W7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -20.32 180) (length 5.08)
        (name "OUT_IGN8" (effects (font (size 1.27 1.27))))
        (number "W8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "Module-mcu-0.5_3_0"
      (rectangle (start 15.24 0) (end 0 -96.52)
        (stroke (width 0)) (fill (type background))
      )
      (pin passive line (at -5.08 -71.12 0) (length 5.08)
        (name "IN_SENS3" (effects (font (size 1.27 1.27))))
        (number "S10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -73.66 0) (length 5.08)
        (name "IN_SENS4" (effects (font (size 1.27 1.27))))
        (number "S11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -78.74 0) (length 5.08)
        (name "IN_KNOCK" (effects (font (size 1.27 1.27))))
        (number "S12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -2.54 0) (length 5.08)
        (name "IN_CRANK" (effects (font (size 1.27 1.27))))
        (number "S13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -7.62 0) (length 5.08)
        (name "IN_VSS" (effects (font (size 1.27 1.27))))
        (number "S14" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -5.08 0) (length 5.08)
        (name "IN_CAM" (effects (font (size 1.27 1.27))))
        (number "S15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -25.4 0) (length 5.08)
        (name "IN_O2S" (effects (font (size 1.27 1.27))))
        (number "S16" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -12.7 0) (length 5.08)
        (name "IN_TPS" (effects (font (size 1.27 1.27))))
        (number "S17" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -20.32 0) (length 5.08)
        (name "IN_CLT" (effects (font (size 1.27 1.27))))
        (number "S18" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -17.78 0) (length 5.08)
        (name "IN_IAT" (effects (font (size 1.27 1.27))))
        (number "S19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -43.18 0) (length 5.08)
        (name "IN_MAP1" (effects (font (size 1.27 1.27))))
        (number "S20" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -45.72 0) (length 5.08)
        (name "IN_MAP2" (effects (font (size 1.27 1.27))))
        (number "S21" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -48.26 0) (length 5.08)
        (name "IN_MAP3" (effects (font (size 1.27 1.27))))
        (number "S22" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -38.1 0) (length 5.08)
        (name "IN_RES3" (effects (font (size 1.27 1.27))))
        (number "S23" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -53.34 0) (length 5.08)
        (name "IN_AUX1" (effects (font (size 1.27 1.27))))
        (number "S24" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -55.88 0) (length 5.08)
        (name "IN_AUX2" (effects (font (size 1.27 1.27))))
        (number "S25" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -58.42 0) (length 5.08)
        (name "IN_AUX3" (effects (font (size 1.27 1.27))))
        (number "S26" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -60.96 0) (length 5.08)
        (name "IN_AUX4" (effects (font (size 1.27 1.27))))
        (number "S27" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -33.02 0) (length 5.08)
        (name "IN_RES1" (effects (font (size 1.27 1.27))))
        (number "S28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -15.24 0) (length 5.08)
        (name "IN_PPS" (effects (font (size 1.27 1.27))))
        (number "S29" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -86.36 0) (length 5.08)
        (name "IN_D1" (effects (font (size 1.27 1.27))))
        (number "S3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -27.94 0) (length 5.08)
        (name "IN_O2S2" (effects (font (size 1.27 1.27))))
        (number "S30" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -35.56 0) (length 5.08)
        (name "IN_RES2" (effects (font (size 1.27 1.27))))
        (number "S31" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -88.9 0) (length 5.08)
        (name "IN_D2" (effects (font (size 1.27 1.27))))
        (number "S4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -91.44 0) (length 5.08)
        (name "IN_D3" (effects (font (size 1.27 1.27))))
        (number "S5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -93.98 0) (length 5.08)
        (name "IN_D4" (effects (font (size 1.27 1.27))))
        (number "S6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -81.28 0) (length 5.08)
        (name "VIGN" (effects (font (size 1.27 1.27))))
        (number "S7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -66.04 0) (length 5.08)
        (name "IN_SENS1" (effects (font (size 1.27 1.27))))
        (number "S8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -68.58 0) (length 5.08)
        (name "IN_SENS2" (effects (font (size 1.27 1.27))))
        (number "S9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "Module-mcu-0.5_4_0"
      (rectangle (start 35.56 0) (end 0 -25.4)
        (stroke (width 0)) (fill (type background))
      )
      (pin passive line (at 40.64 -15.24 180) (length 5.08)
        (name "IO1" (effects (font (size 1.27 1.27))))
        (number "N12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 40.64 -17.78 180) (length 5.08)
        (name "IO2" (effects (font (size 1.27 1.27))))
        (number "N13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 40.64 -20.32 180) (length 5.08)
        (name "IO3" (effects (font (size 1.27 1.27))))
        (number "N14" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 40.64 -22.86 180) (length 5.08)
        (name "IO4" (effects (font (size 1.27 1.27))))
        (number "N15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -10.16 0) (length 5.08)
        (name "V33" (effects (font (size 1.27 1.27))))
        (number "N16" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 40.64 -10.16 180) (length 5.08)
        (name "VBAT" (effects (font (size 1.27 1.27))))
        (number "N17" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 40.64 -2.54 180) (length 5.08)
        (name "nReset" (effects (font (size 1.27 1.27))))
        (number "N24" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 40.64 -5.08 180) (length 5.08)
        (name "BOOT0" (effects (font (size 1.27 1.27))))
        (number "N28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -2.54 0) (length 5.08)
        (name "V5" (effects (font (size 1.27 1.27))))
        (number "S1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -22.86 0) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "S2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -20.32 0) (length 5.08)
        (name "GNDA" (effects (font (size 1.27 1.27))))
        (number "S32" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -17.78 0) (length 5.08)
        (name "V5A" (effects (font (size 1.27 1.27))))
        (number "S33" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -12.7 0) (length 5.08)
        (name "IGN_V33" (effects (font (size 1.27 1.27))))
        (number "W10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -5.08 0) (length 5.08)
        (name "IGN_V5" (effects (font (size 1.27 1.27))))
        (number "W9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)